{"text_format":"1","workbook":"xlsx","n_sheets":16,"sheets":["Home","NVR","IPC","DVR","HDC","Access Intercom","SolarCam","PTZ","Wi-Fi IP","PoE Switches","PoE Accessories","Accessories","מערכת SHOB ","VMS Hardware","Maitainance file","Sheet1"],"not_rendered":{"charts":0,"images":228,"macros":1,"external_links":2,"defined_names":17,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Home","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[[17,1,17,11],[19,1,19,11],[0,1,1,11],[11,3,11,11],[12,3,12,11],[13,3,13,11],[15,3,15,7],[18,1,18,11]]}

{"sheet":"NVR","index":1,"n_rows":25,"n_cols":17,"rows_kept":25,"cut":false,"hidden":false,"merged":[[0,3,0,15],[1,3,1,11],[1,12,1,15],[2,2,2,15]]}
[null,null,"NVR"]
[]
[]
[{"$f":"IF(AND(IFERROR(SEARCH(\"None PoE\",l0&5,1),0)>=1,IFERROR(SEARCH(\"PoE\",l0&5,1),0)>=1,IFERROR(SEARCH(\"RAID\",l0&5,1),0)>=1,IFERROR(SEARCH(\"Face\",l0&5,1),0)>=1,IFERROR(SEARCH(\"DDA Analytic\",l0&5,1),0)>=1,IFERROR(SEARCH(\"FishEye\",l0&5,1),0)>=1),1,0)","v":0},null,"Model","Free","Description","No. of Channels","Max Resolution","Bandwidth","FPS","Video Outputs","HDD","Audio Input","Audio Output","Dry Contact","Special Features","NDAA","PVP 2025"]
[1,null,"NVR5-4100XN(MM)",null,"H.265 Stand Alone NDAA NVR, 4CH  5MP at 25fps. MM case",4,"5MP","40Mbps/\n64Mbps","25fps 5MP ","HDMI, VGA","1 of 6TB Max","Based on IPC Only","Based on IPC Only","Based on IPC Only","None PoE \nDDA Analytic","Yes",145]
[1,null,"NVR5-4100PXN(MM)",null,"H.265 Stand Alone NDAA NVR, 4CH  5MP at 25fps, MM case with PoE",4,"5MP","40Mbps/\n64Mbps","25fps 5MP ","HDMI, VGA","1 of 6TB Max","Based on IPC Only","Based on IPC Only","Based on IPC Only","with PoE \nDDA Analytic","Yes",235]
[1,null,"NVR8-4100PN-V2",null,"H.265 Stand Alone NDAA NVR, 4CH  8MP at 25fps,  Small 1U case with PoE",4,"8MP","80Mbps/\n80Mbps","25fps 8MP ","HDMI 4K, VGA","1 of 10TB Max","1+IPC","1+IPC","Based on IPC Only","with PoE \nDDA Analytic\nLPR\nCheak Point Protect\nAI Engine","Yes",360]
[1,null,"NVR5-8200XN(MM)",null,"H.265 Stand Alone NDAA NVR, 8CH  5MP at 25fps. MM case",8,"5MP","64Mbps/\n64Mbps","25fps 5MP ","HDMI, VGA","1 of 6TB Max","Based on IPC Only","Based on IPC Only","Based on IPC Only","None PoE \nDDA Analytic","Yes",177]
[1,null,"NVR5-8200PXN(MM)",null,"H.265 Stand Alone NDAA NVR, 8CH  5MP at 25fps, MM case with PoE",8,"5MP","64Mbps/\n64Mbps","25fps 5MP ","HDMI, VGA","1 of 6TB Max","Based on IPC Only","Based on IPC Only","Based on IPC Only","with PoE \nDDA Analytic","Yes",330]
[1,null,"NVR8-8200N-V2",null,"H.265 Stand Alone NDAA NVR, 8CH  8MP at 25fps. Small 1U case",8,"8MP","80Mbps/\n80Mbps","25fps 8MP ","HDMI 4K, VGA","1 of 8TB Max","1+IPC","1+IPC","Based on IPC Only","None PoE \nDDA Analytic\nLPR\nCheck Point Protect\nAI Engine","Yes",311]
[1,null,"NVR8-8200PN-V2",null,"H.265 Stand Alone NDAA NVR, 8CH  8MP at 25fps,Small 1U case with PoE",8,"8MP","80Mbps/\n80Mbps","25fps 8MP ","HDMI 4K, VGA","1 of 10TB Max","1+IPC","1+IPC","Based on IPC Only","with  PoE \nDDA Analytic\nLPR\nCheck Point Protect\nAI Engine","Yes",498]
[1,null,"NVR12-8200FAN",null,"H.265 Stand Alone NDAA NVR, 8CH  12MP at 25fps. Small 1U case",8,"12MP","80Mbps/\n80Mbps","25fps 12MP ","HDMI 4K, VGA","1 of 10TB Max","1+IPC","1+IPC","In- 8+IPC Out- 4+IPC","None PoE\nFace \nDDA Analytic  FishEye\nLPR\nAI Engine","Yes",410]
[1,null,"NVR12-8200PFAN",null,"H.265 Stand Alone NDAA NVR, 8CH PoE 12MP at 25fps. Small 1U case with PoE",8,"12MP","80Mbps/\n80Mbps","25fps 12MP ","HDMI 4K, VGA","1 of 10TB Max","1+IPC","1+IPC","In- 8+IPC Out- 4+IPC","with PoE \nFace \nDDA Analytic  FishEye\nLPR\nAI Engine","Yes",673]
[1,null,"NVR8-16400AN(1U)-V2",null,"H.265 Stand Alone NDAA NVR, 16CH  8MP at 25fps. 1U case",16,"8MP","96Mbps/\n96Mbps","25fps 8MP ","HDMI 4K, VGA","2 of 10TB Max","1+IPC","1+IPC","In- 4+IPC Out- 1+IPC","None PoE\nDDA Analytic\nLPR\nCheck Point Protect\nAI Engine","Yes",343]
[1,null,"NVR12-16400FAN(1U)",null,"H.265 Stand Alone NDAA NVR, 16CH  12MP at 25fps. 1U case, support Face recognition",16,"12MP","160Mbps/\n160Mbps","25fps 12MP ","HDMI 4K, VGA","2 of 10TB Max","1+IPC","1+IPC","In- 8+IPC Out- 4+IPC","None PoE\n Face \nDDA Analytic  FishEye\nLPR\nAI Engine","Yes",583]
[1,null,"NVR12-16400PFAN(1U)",null,"H.265 Stand Alone NDAA NVR, 16CH PoE  12MP at 25fps. 1U case, support Face recognition",16,"12MP","160Mbps/\n160Mbps","25fps 12MP ","HDMI 4K, VGA","2 of 10TB Max","1+IPC","1+IPC","In- 8+IPC Out- 4+IPC"," with PoE \nFace \nDDA Analytic  FishEye\nLPR\nAI Engine","Yes",960]
[1,null,"NVR12-32800FN-16P(2U)",null,"H.265 Stand Alone NDAA NVR, 32CH  8MP at 25fps, 2U case with 16CH PoE, support Face recognition",32,"12MP","192Mbps/\n192Mbps","25fps 12MP ","2 of HDMI, 4K, VGA","8 of 10TB Max","1+IPC","1+IPC","In- 16+IPC Out- 4+IPC","with PoE \nFace \nDDA Analytic  FishEye\nLPR\nCheck Point Protect\nAI Engine","Yes",1416]
[1,null,"NVR12-32800FAN(1U)",null,"H.265 Stand Alone NDAA NVR, 32CH  12MP at 20fps, 1U case, support Face recognition",32,"12MP","192Mbps/\n192Mbps","25fps 12MP ","2 of HDMI, 4K, VGA","2 of 10TB Max","1+IPC","1+IPC","In- 8+IPC Out- 4+IPC"," None*PoE \nFace \nDDA Analytic FishEye \nLPR\n2*Ethernet\nCheck Point Protect\nAI Engine","Yes",732]
[1,null,"NVR12-32800RFAN(2U)",null,"H.265 Stand Alone NDAA NVR, 32CH  12MP at 20fps, 2U case, support Face recognition, with RAID",32,"12MP","320Mbps/\n256Mbps","25fps 12MP ","2 of HDMI, 4K, VGA","8 of 10TB Max","1+IPC","1+IPC","In- 16+IPC Out- 4+IPC"," None*PoE \nFace \nDDA Analytic FishEye \nLPR\n2*Ethernet\nCheck Point Protect\nAI Engine","Yes",1322]
[1,null,"NVR16-641600RFAN(2U)",null,"H.265 Stand Alone NDAA NVR, 64CH 16MP,support Face recognition, with RAID,2U case",64,"16MP","640Mbps/\n640Mbps","25fps 16MP ","HDMI, 8K, VGA","8 of 8TB Max","1+IPC","1+IPC","In- 16+IPC Out- 8+IPC"," None PoE  \nDDA Analytic  FishEye\nLPR \nRaid 2*Ethernet\nAI Engine","Yes",1755]
[1,null,"NVR16-128RFAN(3U)",null,"H.265 Stand Alone NDAA NVR, 128CH 16MP,support Face recognition, with RAID,3U case",128,"16MP","768Mbps/\n768Mbps","25fps 16MP ","4 HDMI, 8K, VGA","16 of 8TB Max","1+IPC","1+IPC","In- 24+IPC Out- 4+IPC"," None PoE  \nDDA Analytic  FishEye\nLPR \nRaid 2*Ethernet\nAI Engine","Yes",5472]
[1]
[1]
[1]
[1]

{"sheet":"IPC","index":2,"n_rows":111,"n_cols":20,"rows_kept":111,"cut":false,"hidden":false,"merged":[[0,4,0,18],[1,4,1,13],[1,14,1,18],[2,3,2,18]]}
[null,null,null,"IPC"]
[]
[]
[null,null,"R","Model","free text","Series","Description","Resolution","Housing","WDR","Lens Type","Lens Focal","Protection","IR range","Juntion box","Special features","Analytic","NDAA","Remarks","PVP 2025"]
[1,null,null,"DH-320IPBN-28",null,"B-Sight","Camera- H.265 Basic-Series,Dual-light Turret/Dome, IR 20M(1 LED Array),2.8mm lens, 2M with PoE","2MP","Turret/Dome","DWDR","Fixed","2.8mm (93°)","IP67","20M","PR-JB12IP66 - PR-JB12IP64 - PR-WB-A","Made of aluminum alloy and polycarbonate\nBuilt-in Mic","Camera Tampering \nStandard- Line Crossing \nStandard- Sterile Area,\nDDA- Line Crossing \nDDA- Sterile Area","Yes",null,95]
[1,1,null,"BSH-320IPBN-28",null,"B-Sight","Camera- H.265 Basic-Series, Dual-light ,Bullet, IR 20M(1 LED Array),2.8mm lens, 2M with PoE","2MP","Bullet","DWDR","Fixed","2.8mm (93°)","IP67","20M","PR-JB12IP66\n PR-JB12IP64 ","Made of aluminum alloy and polycarbonate\nBuilt-in Mic","Camera Tampering \nStandard- Line Crossing \nStandard- Sterile Area,\nDDA- Line Crossing \nDDA- Sterile Area","Yes",null,95]
[1,1,null,"DH-340IPBN-28",null,"B-Sight","Camera- H.265 Basi-Series,Dual-light Turret/Dome, IR 20M(1 LED Array),2.8mm lens, 4M with Po","4MP","Turret/Dome","DWDR","Fixed","2.8mm (93°)","IP67","20M","PR-JB12IP66 - PR-JB12IP64 - PR-WB-A","Made of aluminum alloy and polycarbonate\nBuilt-in Mic","Camera Tampering \nStandard- Line Crossing \nStandard- Sterile Area,\nDDA- Line Crossing \nDDA- Sterile Area","Yes",null,125]
[1,1,null,"BSH-340IPBN-28",null,"B-Sight","Camera- H.265 Basic-Series, Dual-light,Bullet, IR 20M(1 LED Array),2.8mm lens, 4M with PoE","4MP","Bullet","DWDR","Fixed","2.8mm (93°)","IP67","20M","PR-JB12IP66 \nPR-JB12IP64","Made of aluminum alloy and polycarbonate\nBuilt-in Mic","Camera Tampering \nStandard- Line Crossing \nStandard- Sterile Area,\nDDA- Line Crossing \nDDA- Sterile Area","Yes",null,125]
[1,1,null,"DI-320IPSN-28-V4",null,"S-Sight","Camera- H.265 S-Sight Series,, Dome/Turret, IR 20M(1 LED Array), 2.8mm Lens 2M with PoE","2MP","Turret/Dome","True WDR","Fixed","2.8mm (104°)","IP67","20M","PR-DJB12IP66/\nPR-JB12IP66/\nPR-JB12IP64/ PR-WB-A","Audio In\nBuilt-in Mic \nSD Card\nCheck Point Protect","Camera Tampering \nStandard- Line Crossing \nStandard- Sterile Area,\nDDA- Line Crossing \nDDA- Sterile Area","Yes",null,124]
[1,1,null,"DI-320IPSN-28-G-V2",null,"S-Sight","Camera- H.265 S-Sight Series,, Dome/Turret, IR 20M(1 LED Array), 2.8mm Lens 2M with PoE Grey","2MP","Turret/Dome","DWDR","Fixed","2.8mm (104°)","IP67","20M","PR-JB12IP66-G/ PR-WB-A-G","Audio In\nSD Card\nBuilt-in Mic","Camera Tampering \nStandard- Line Crossing \nStandard- Sterile Area\nDDA- Line Crossing \nDDA- Sterile Area","Yes","EOL, replaced by DH-320IPSN-28-G",125]
[1,null,null,"DH-320IPSN-28-G",null,"S-Sight","2MP Fixed Lens Dome/Turret Camera with Hybrid LED and DDA1 Analytics","2MP","Turret/Dome","True WDR","Fixed","2.8mm (104°)","IP67","20M","PR-JB12IP66-G/ PR-WB-A-G","Hybrid Light\nAudio In\nSD Card\nBuilt-in Mic\nCheck Point Protect","Camera Tampering \nStandard- Line Crossing \nStandard- Sterile Area\nDDA- Line Crossing \nDDA- Sterile Area","Yes","New Model",129]
[1,1,null,"DI-320IPSN-VF-V4",null,"S-Sight","Camera- H.265 S-Sight Series, Dome/Turret IR 40M(2 LED Array), 2.8-12mm lens, 2M with PoE","2MP","Turret/Dome","True WDR","Vari-Focal","2.8-12mm (96-33°)","IP67","40M","PR-DJB14IP66/\nPR-JB14IP66/\nPR-JB14IP64/\nPR-WB-A","Audio In\nSD Card\nBuilt-in Mic\nCheck Point Protect","Camera Tampering \nStandard- Line Crossing \nStandard- Sterile Area\nDDA- Line Crossing \nDDA- Sterile Area","Yes","EOL, replaced by DH-320IPSN-MVF",187]
[1,null,null,"DH-320IPSN-VF",null,"S-Sight","2MP Vari-Focal Lens Dome/Turret Camera with Hybrid LED and DDA1 Analytics","2MP","Turret/Dome","True WDR","Vari-Focal","2.8-12mm (96-33°)","IP67","40M","PR-DJB14IP66/\nPR-JB14IP66/\nPR-JB14IP64/\nPR-WB-A","Hybrid Light\nAudio In\nSD Card\nBuilt-in Mic\nCheck Point Protect","Camera Tampering \nStandard- Line Crossing \nStandard- Sterile Area\nDDA- Line Crossing \nDDA- Sterile Area","Yes","New Model",193]
[1,1,null,"DI-320IPSN-VF-G",null,"S-Sight","Camera- H.265 S-Sight Series, Dome/Turret IR 40M(2 LED Array), 2.8-12mm lens, 2M with PoE, Grey","2MP","Turret/Dome","DWDR","Vari-Focal","2.8-12mm (88°-34.8°)","IP67","40M","PR-JB14IP66-G/\nPR-WB-A-G","Built-in Mic \nSD Card","Camera Tampering \nStandard- Line Crossing \nStandard- Sterile Area","Yes","call for special offer",190]
[1,1,null,"I2-320IPSN-28-V4",null,"S-Sight","Camera- H.265 S-Sight Series, Bullet, IR 20M(1 LED Array),2.8mm lens, 2M with PoE","2MP","Bullet","True WDR","Fixed","2.8mm (105°)","IP67","20M","PR-JB12IP66/\nPR-JB12IP64","Audio In\nSD Card\nCheck Point Protect","Camera Tampering \nStandard- Line Crossing \nStandard- Sterile Area\nDDA- Line Crossing \nDDA- Sterile Area","Yes",null,127]
[1,1,null,"I2-320IPSN-28-G",null,"S-Sight","Camera- H.265 S-Sight Series, Bullet, IR 20M(1 LED Array),2.8mm lens, 2M with PoE,grey","2MP","Bullet","DWDR","Fixed","2.8mm (107°)","IP67","20M","PR-JB12IP66/\nPR-JB12IP64","SD Card","Camera Tampering \nStandard- Line Crossing \nStandard- Sterile Area","Yes","call for special offer",130]
[1,1,null,"I2-320IPSN-28-G-V2",null,"S-Sight","Camera- H.265 S-Sight Series, Bullet, IR 20M(1 LED Array),2.8mm lens, 2M with PoE,grey","2MP","Bullet","DWDR","Fixed","2.8mm (107°)","IP67","20M","PR-JB12IP66/\nPR-JB12IP65","Audio In\nSD Card","Camera Tampering \nStandard- Line Crossing \nStandard- Sterile Area\nDDA- Line Crossing \nDDA- Sterile Area","Yes","call for special offer",130]
[1,1,null,"I4-320IPSN-28-V4",null,"S-Sight","Camera- H.265 S-Sight Series, Bullet, IR 40M(2 LED Array),2.8mm Lens, 2M with PoE","2MP","Bullet","True WDR","Fixed","2.8mm (104°)","IP67","40M","PR-JB12IP66/\nPR-JB12IP64","Audio In\nSD Card\nCheck Point Protect","Camera Tampering \nStandard- Line Crossing \nStandard- Sterile Area\nDDA- Line Crossing \nDDA- Sterile Area","Yes","call for special offer",142]
[1,1,null,"I4-320IPSN-VF-V4",null,"S-Sight","Camera- H.265 S-Sight Series, Bullet, IR 40M(2 LED Array),2.8-12mm lens, 2M with PoE","2MP","Bullet","True WDR","Vari-Focal","2.8-12mm  (100°-33°)","IP67","40M","PR-JB12IP66/\nPR-JB12IP64","Audio In\nSD Card\nBuilt-in Mic\nCheck Point Protect","Camera Tampering \nStandard- Line Crossing \nStandard- Sterile Area\nDDA- Line Crossing \nDDA- Sterile Area","Yes","EOL, replaced by BMH-320IPSN-VF",188]
[1,null,null,"BMH-320IPSN-VF",null,"S-Sight","2MP Vari-Focal Lens Bullet Camera with Hybrid LED and DDA1 Analytics","2MP","Bullet","True WDR","Vari-Focal","2.8-12mm  (100°-33°)","IP67","40M","PR-JB12IP66/\nPR-JB12IP64","Hybrid Light\nAudio In\nSD Card\nBuilt-in Mic\nCheck Point Protect","Camera Tampering \nStandard- Line Crossing \nStandard- Sterile Area\nDDA- Line Crossing \nDDA- Sterile Area","Yes","New Model",191]
[1,1,null,"DI-340IPSN-28-V2",null,"S-Sight","Camera- H.265 S-Sight Series,, Dome/Turret IR 20M(1 LED Array), 2.8mm Lens, 4M with PoE","4MP","Turret/Dome","True WDR","Fixed","2.8mm (102°)","IP67","20M","PR-DJB12IP66/\nPR-JB12IP66/\nPR-JB12IP64/ PR-WB-A","Audio In\nSD Card\nBuilt-in Mic","Camera Tampering \nStandard- Line Crossing \nStandard- Sterile Area","Yes","EOL, repalce by DH-340IPSN-28",172]
[1,null,null,"DH-340IPSN-28",null,"S-Sight","Camera- S-Sight , Dome/Turret, Hybrid light Illumination, 2.8mm Lens, Checkpoint embedded,4MP","4MP","Turret/Dome","True WDR","Fixed","2.8mm (93°)","IP67","20M","PR-DJB12IP66/\nPR-JB12IP66/\nPR-JB12IP64/ PR-WB-A","Hybrid Light\nAudio In\nSD Card\nBuilt-in Mic\nCheck Point Protect","Camera Tampering \nStandard- Line Crossing \nStandard- Sterile Area\nDDA- Line Crossing \nDDA- Sterile Area","Yes","New Model",180]
[1,null,null,"DH-340ADSN-28",null,"S-Sight","S-Sight,Hybrid light,Active deterrence,Dome/Turret,Illumination20M,2.8mmLens,Checkpoint embedded,4MP","4MP","Turret/Dome","True WDR","Fixed","2.8mm (94°)","IP67","30M","PR-DJB12IP66/\nPR-JB12IP66/\nPR-JB12IP64/ PR-WB-A","Hybrid Light\nAudio In\nAudio Out \nBuilt-in Mic \nBuilt-in speaker\nRed/Blue Strobe Light\nSD Card\nCheck Point Protect","Camera Tampering \nStandard- Line Crossing \nStandard- Sterile Area\nDDA- Line Crossing \nDDA- Sterile Area","Yes",null,294]
[1,null,null,"DH-340IPSN-28-G",null,"S-Sight","Camera- S-Sight , Dome/Turret, Hybrid light Illumination, 2.8mm Lens, Checkpoint embedded,4MP","4MP","Turret/Dome","True WDR","Fixed","2.8mm (93°)","IP67","20M","PR-JB12IP66/\nPR-JB12IP64/ PR-WB-A","Hybrid Light\nAudio In\nSD Card\nBuilt-in Mic\nCheck Point Protect","Camera Tampering \nStandard- Line Crossing \nStandard- Sterile Area\nDDA- Line Crossing \nDDA- Sterile Area","Yes",null,179]
[1,null,null,"DH-340IPSN-MVF",null,"S-Sight","Camera- S-Sight , Dome/Turret, Hybrid light Illumination, Motorized 2.8-12mm lens, CheckPoint embedded,4MP","4MP","Turret/Dome","True WDR","Motorized Vari-Focal","2.8-12mm\n(89°-31°)","IP67","40M","PR-DJB14IP66/\nPR-JB14IP66/\nPR-JB14IP64/\nPR-WB-A","Hybrid Light\nAudio In\nSD Card\nBuilt-in Mic\nCheck Point Protect","Camera Tampering \nStandard- Line Crossing \nStandard- Sterile Area\nDDA- Line Crossing \nDDA- Sterile Area","Yes",null,285]
[1,null,null,"DH-340IPSN-MVF-G",null,"S-Sight","4MP MVF Lens Dome/Turret Camera with Hybrid LED and DDA1 Analytics","4MP","Turret/Dome","True WDR","Motorized Vari-Focal","2.8-12mm\n(94°-35.7°)","IP67","40M","PR-JB14IP66-G/\nPR-WB-A-G","Hybrid Light\nAudio In\nSD Card\nBuilt-in Mic\nCheck Point Protect","Camera Tampering \nStandard- Line Crossing \nStandard- Sterile Area\nDDA- Line Crossing \nDDA- Sterile Area","Yes",null,288]
[1,1,null,"I2-340IPSN-28-V2",null,"S-Sight","Camera- H.265 S-Sight Series, Bullet, IR 20M(1 LED Array),2.8mm lens, 4M with PoE","4MP","Bullet","True WDR","Fixed","2.8mm (110°)","IP67","20M","PR-JB12IP66/\nPR-JB12IP65","Audio In\nSD Card","Camera Tampering \nStandard- Line Crossing \nStandard- Sterile Area\nDDA- Line Crossing \nDDA- Sterile Area","Yes",null,171]
[1,1,null,"I2-340IPSN-28-G-V2",null,"S-Sight","Camera- H.265 S-Sight Series, Bullet, IR 20M(1 LED Array),2.8mm lens, 4M with PoE,grey","4MP","Bullet","True WDR","Fixed","2.8mm (110°)","IP67","20M","PR-JB12IP66/\nPR-JB12IP64","Audio In\nSD Card","Camera Tampering \nStandard- Line Crossing \nStandard- Sterile Area\nDDA- Line Crossing \nDDA- Sterile Area","Yes",null,174]
[null,null,null,"BMH-340IPSN-28",null,"S-Sight","Camera- H.265 S-Sight Series, Hybrid light,Bullet, IR 40M(2 LED Array),2.8mm Lens, 4M with PoE","4MP","Bullet","True WDR","Fixed","2.8mm (94°)","IP67","20M","PR-JB12IP66/\nPR-JB12IP64","Hybrid Light\nAudio In\nSD Card\nBuilt-in Mic\nCheck Point Protect","Camera Tampering \nStandard- Line Crossing \nStandard- Sterile Area\nDDA- Line Crossing \nDDA- Sterile Area","Yes","New Model",213]
[1,1,null,"I4-340IPSN-MVF-V2",null,"S-Sight","Camera- H.265 S-Sight Series, Bullet, IR 40M(2 LED Array), Motorized 2.8-12mm lens, 4M with PoE","4MP","Bullet","True WDR","Motorized Vari-Focal","2.8-12mm\n(94°-35.7°)","IP67","40M","PR-JB12IP66/\nPR-JB12IP64","Audio In\nSD Card","Camera Tampering \nStandard- Line Crossing \nStandard- Sterile Area\nDDA- Line Crossing \nDDA- Sterile Area","Yes","EOL, replaced by BMH-340IPSN-MVF",284]
[1,null,null,"BMH-340IPSN-MVF",null,"S-Sight","4MP MVF Lens Bullet Camera with Hybrid LED and DDA1 Analytics","4MP","Bullet","True WDR","Motorized Vari-Focal","2.8-12mm\n(94°-35.7°)","IP67","40M","PR-JB12IP66/\nPR-JB12IP64","Hybrid Light\nAudio In\nSD Card\nBuilt-in Mic\nCheck Point Protect","Camera Tampering \nStandard- Line Crossing \nStandard- Sterile Area\nDDA- Line Crossing \nDDA- Sterile Area","Yes","New Model",288]
[1,null,null,"BMH-340ADSN-28",null,"S-Sight","S-Sight,,Active deterrence, Bullet,Hybrid light Illumination, 2.8mmLens, CheckPoint embedded,4MP","4MP","Bullet","True WDR","Fixed","2.8mm (94°)","IP67","30M","PR-JB12IP66/\nPR-JB12IP64","Hybrid Light\nAudio In\nAudio Out \nBuilt-in Mic \nBuilt-in speaker\nRed/Blue Strobe Light\nSD Card\nCheck Point Protect","Camera Tampering \nStandard- Line Crossing \nStandard- Sterile Area\nDDA- Line Crossing \nDDA- Sterile Area","Yes",null,277]
[1,null,null,"DAH-340IPSN-28",null,"S-Sight","S-Sight, Dome/Turret, Hybrid light Illumination, 2.8 lens, Checkpoint embedded, 4MP","4MP","Dome Anti-Vandal","True WDR","Fixed","2.8mm (93°)","IP67/\nIK10","20M","PR-JB12IP66 / PR-ICB21 / \nPR-WB-A","Hybrid Light\nAudio In\nSD Card\nBuilt-in Mic\nCheck Point Protect","Camera Tampering \nStandard- Line Crossing \nStandard- Sterile Area\nDDA- Line Crossing \nDDA- Sterile Area","Yes",null,215]
[1,1,null,"DMA-350IPSN-28-V4",null,"S-Sight","Camera-H.265 S-Sight Series, Mini dome, IR 10M, 2.8mm Lens 5MP with PoE","5MP","Dome Anti-Vandal","True WDR","Fixed","2.8mm (108°)","IP67/\nIK10","10M","PR-B10BJB / \nPR-WB-A","Audio in\nSD Card\nBuild-in Mic\nCheck Point Protect","Camera Tampering \nStandard- Line Crossing \nStandard- Sterile Area\nDDA- Line Crossing \nDDA- Sterile Area","Yes",null,225]
[1,1,null,"DI-380IPSN-28-V3",null,"S-Sight","Camera- H.265 S-Sight Series,, Dome/Turret IR 20M(1 LED Array), 2.8mm Lens 8M with PoE","8MP","Turret/Dome","True WDR","Fixed","2.8mm (108.9°)","IP67","20M","PR-DJB12IP66/\nPR-JB12IP66/\nPR-JB12IP64/ PR-WB-A","Audio In\nSD Card\nBuilt-in Mic\nCheck Point Protect","Camera Tampering \nStandard- Line Crossing \nStandard- Sterile Area\nDDA- Line Crossing \nDDA- Sterile Area","Yes","EOL, replace by DH-380IPSN-28",327]
[1,null,null,"DH-380IPSN-28",null,"S-Sight","Camera- S-Sight , Dome/Turret, Hybrid light Illumination, 2.8mm Lens, Checkpoint embedded,8MP","8MP","Turret/Dome","True WDR","Fixed","2.8mm (103°)","IP67","20M","PR-DJB12IP66/\nPR-JB12IP66/\nPR-JB12IP64/ PR-WB-A","Hybrid Light\nAudio In\nSD Card\nBuilt-in Mic\nCheck Point Protect","Camera Tampering \nStandard- Line Crossing \nStandard- Sterile Area\nDDA- Line Crossing \nDDA- Sterile Area","Yes","New Model",330]
[1,null,null,"DH-380IPSN-28-G",null,"S-Sight","Camera- S-Sight , Dome/Turret, Hybrid light, Illumination.2.8mm Lens, Checkpoint embedded,8MP","8MP","Turret/Dome","True WDR","Fixed","2.8mm (103°)","IP67","20M","PR-JB12IP66-G/\nPR-WB-A-G","Hybrid Light\nAudio In\nSD Card\nBuilt-in Mic\nCheck Point Protect","Camera Tampering \nStandard- Line Crossing \nStandard- Sterile Area\nDDA- Line Crossing \nDDA- Sterile Area","Yes",null,325]
[1,1,null,"DI-380IPSN-MVF-V3",null,"S-Sight","Camera- H.265 S-Sight Series, Dome/Turret IR 40M(2 LED Array), Motorized  2.8-12mm lens, 8M with PoE","8MP","Turret/Dome","True WDR","Motorized Vari-Focal","2.8-12mm\n(102°-32.1°)","IP67","40M","PR-DJB14IP66/\nPR-JB14IP66/\nPR-JB14IP64/\nPR-WB-A","Audio In\nSD Card\nBuilt-in Mic\nCheck Point Protect","Camera Tampering \nStandart- Line Crossing \nStandart- Sterile Area\nDDA- Line Crossing \nDDA- Sterile Area","Yes","EOL, replace by DH-380IPSN-MVF",445]
[null,null,null,"DH-380IPSN-MVF",null,"S-Sight","S-Sight,Hybrid light,Dome/Turret Illumination 40M, Motorized 2.8-12mm lens,6MP","8MP","Turret/Dome","True WDR","Motorized Vari-Focal","2.8-12mm\n(102°-32.1°)","IP67","20M","PR-JB12IP66-G/\nPR-WB-A-G","Hybrid Light\nAudio In\nSD Card\nBuilt-in Mic\nCheck Point Protect","Camera Tampering \nStandard- Line Crossing \nStandard- Sterile Area\nDDA- Line Crossing \nDDA- Sterile Area","Yes","New Model",448]
[1,1,null,"DI-380IPSN-MVF-G-V3",null,"S-Sight","Camera- H.265 S-Sight Series, Dome/Turret IR 40M(2 LED Array), Motorized  2.8-12mm lens, 8M with PoE","8MP","Turret/Dome","True WDR","Motorized Vari-Focal","2.8-12mm\n(102.7°-32.2°)","IP67","40M","PR-JB14IP66/\nPR-JB14IP64/\nPR-WB-A","Audio In\nSD Card\nBuilt-in Mic\nCheck Point Protect","Camera Tampering \nStandart- Line Crossing \nStandart- Sterile Area\nDDA- Line Crossing \nDDA- Sterile Area","Yes","EOL, replace by DH-380IPSN-MVF-G",445]
[null,null,null,"DH-380IPSN-MVF-G",null,"S-Sight","Camera- H.265 S-Sight Series, Dome/Turret IR 40M(2 LED Array), Motorized  2.8-12mm lens, 8M with PoE","8MP","Turret/Dome","True WDR","Motorized Vari-Focal","2.8-12mm\n(94°-35.7°)","IP67","40M","PR-JB14IP66-G/\nPR-WB-A-G","Hybrid Light\nAudio In\nSD Card\nBuilt-in Mic\nCheck Point Protect","Camera Tampering \nStandard- Line Crossing \nStandard- Sterile Area\nDDA- Line Crossing \nDDA- Sterile Area","Yes","New Model",448]
[1,null,null,"BMH-380IPSN-28",null,"S-Sight","8MP Fixed Lens Bullet Camera with Hybrid LED and DDA1 Analytics","8MP","Bullet","True WDR","Fixed","2.8mm (101°)","IP67","40M","PR-JB12IP66/\nPR-JB12IP64","Hybrid Light\nAudio In\nSD Card\nBuilt-in Mic\nCheck Point Protect","Camera Tampering \nStandart- Line Crossing \nStandart- Sterile Area\nDDA- Line Crossing \nDDA- Sterile Area","Yes",null,354]
[1,null,null,"BMH-380IPSN-MVF",null,"S-Sight","8MP MVF Lens Bullet Camera with Hybrid LED and DDA1 Analytics","8MP","Bullet","True WDR","Motorized Vari-Focal","2.8-12mm\n(99°-34°)","IP67","40M","PR-JB12IP66/\nPR-JB12IP64","Hybrid Light\nAudio In\nSD Card\nBuilt-in Mic\nCheck Point Protect","Camera Tampering \nStandart- Line Crossing \nStandart- Sterile Area\nDDA- Line Crossing \nDDA- Sterile Area","Yes",null,445]
[1,1,null,"DMA-320IPEN-28-V4",null,"Eye-Sight","Camera-H.265 Eye-Sight Series, Mini dome, IR 10M, 2.8mm Lens 2MP with PoE","2MP","Dome Anti-Vandal","True WDR","Fixed","2.8mm (103°)","IP67/\nIK10","10M","PR-B10BJB / \nPR-WB-A","Audio In \nBuilt-in Mic\nSD Card\nCheck Point Protect","Camera Tampering \nDDA- Line Crossing \nDDA- Sterile Area\nDDA- Object Counting (line)\nDDA- Object Counting (area)\nItem monitoring\nHeat Map\nFace Detection,\nDDA2- Advanced Object Classification","Yes",null,253]
[1,1,null,"DAI-320IPEN-28-V4",null,"Eye-Sight","Camera-H.265 Eye-Sight Series, Anti-Vandal, IR 20M(3 LED Array), 2.8mm lens , 2M with PoE","2MP","Dome Anti-Vandal","True WDR","Fixed","2.8mm (99°)","IP67/\nIK10","20M","PR-JB12IP66 / PR-ICB21 / PR-WB-A","Audio In \nAudio Out \nI/O\nSD Card\nBuilt-in Mic\nCheck Point Protect","Camera Tampering \nDDA- Line Crossing \nDDA- Sterile Area\nDDA- Object Counting (line)\nDDA- Object Counting (area)\nItem monitoring\nHeat Map\nFace Detection,\nDDA2- Advanced Object Classification","Yes","call for special offer",250]
[1,null,null,"DAI-320IPEN-MVF-V4",null,"Eye-Sight","Camera-H.265 Eye-Sight Series, Anti-Vandal, IR 40M(2 LED Array), Motorized2.8-12mm lens, 2M with PoE","2MP","Dome Anti-Vandal","True WDR","Motorized Vari-Focal","2.8-12mm\n(106°-30°)","IP67/\nIK10","40M","PR-JB14IP66 / PR-ICB23","Audio In \nAudio Out \nI/O\nSD Card\nBuilt-in Mic\nCheck Point Protect","Camera Tampering \nDDA- Line Crossing \nDDA- Sterile Area\nDDA- Object Counting (line)\nDDA- Object Counting (area)\nItem monitoring\nHeat Map\nFace Detection,\nDDA2- Advanced Object Classification","Yes",null,360]
[1,1,null,"DI-320IPEN-28",null,"Eye-Sight","Camera- H.265 Eye-Sight Series,, Dome/Turret IR 20M(1 LED Array), 2.8mm Lens, 2M with PoE","2MP","Turret/Dome","True WDR","Fixed","2.8mm (108°)","IP67","20M","PR-DJB12IP66/\nPR-JB12IP66/\nPR-JB12IP64/ PR-WB-A","Audio In \nBuilt-in Mic\nSD Card","Camera Tampering \nDDA- Line Crossing \nDDA- Sterile Area\nDDA- Object Counting (line)\nDDA- Object Counting (area)\nItem monitoring\nHeat Map\nFace Detection \nDDA2- Advanced Object Classification\nDDA- Audio Exception\nDDA- Illegal Parking Detection\nDDA- Loitering Detection","Yes",null,238]
[1,1,null,"DI-320IPEN-MVF-V4",null,"Eye-Sight","Camera- H.265 Eye-Sight Series, Dome/Turret IR 40M(2 LED Array), Motorized  2.8-12mm lens, 2M with P","2MP","Turret/Dome","True WDR","Motorized Vari-Focal","2.8-12mm\n(100°-31°)","IP67","40M","PR-DJB14IP66/\nPR-JB14IP66/\nPR-JB14IP64/\nPR-WB-A","Audio In \nAudio Out \nI/O\nSD Card\nBuilt-in Mic\nCheck Point Protect","Camera Tampering \nDDA- Line Crossing \nDDA- Sterile Area\nDDA- Object Counting (line)\nDDA- Object Counting (area)\nItem monitoring\nHeat Map\nFace Detection \nDDA2- Advanced Object Classification\nDDA- Audio Exception\nDDA- Illegal Parking Detection\nDDA- Loitering Detection","Yes",null,327]
[1,1,null,"I4-320IPEN-36-V4",null,"Eye-Sight","Camera- H.265 Eye-Sight Series, Bullet, IR 40M(2 LED Array), 3.6mm lens, 2M with PoE","2MP","Bullet","True WDR","Fixed","3.6mm (86°)","IP67","40M","PR-JB12IP66/\nPR-JB12IP64","Audio In\nSD Card\nCheck Point Protect","Camera Tampering \nDDA- Line Crossing \nDDA- Sterile Area\nDDA- Object Counting (line)\nDDA- Object Counting (area)\nItem monitoring\nHeat Map\nFace Detection,\nDDA2- Advanced Object Classification","Yes","call for special offer",257.03811000000002]
[1,1,null,"I4-320IPEN-MVF-V4",null,"Eye-Sight","Camera- H.265 Eye-Sight Series, Bullet, IR 40M(2 LED Array), Motorized 2.8-12mm lens, 2M with PoE","2MP","Bullet","True WDR","Motorized Vari-Focal","2.8-12mm\n(103°-32°)","IP67","40M","PR-JB12IP66/\nPR-JB12IP64","Audio In \nAudio Out \nI/O\nSD Card\nBuilt-in Mic\nCheck Point Protect","Camera Tampering \nDDA- Line Crossing \nDDA- Sterile Area\nDDA- Object Counting (line)\nDDA- Object Counting (area)\nItem monitoring\nHeat Map\nFace Detection \nDDA2- Advanced Object Classification\nDDA- Audio Exception\nDDA- Illegal Parking Detection\nDDA- Loitering Detection","Yes",null,360]
[1,1,null,"I6-320IPEN-MVF-V4",null,"Eye-Sight","Camera- H.265 Eye-Sight Series, Bullet, IR 60M(4 LED Array), Motorized 2.8-12mm lens, 2M with PoE","2MP","Bullet","True WDR","Motorized Vari-Focal","2.8-12mm\n(103°-32°)","IP67","60M","PR-JB14IP66/\nPR-JB14IP64","Audio In \nAudio Out \nI/O\nSD Card\nBuilt-in Mic\nCheck Point Protect","Camera Tampering \nDDA- Line Crossing \nDDA- Sterile Area\nDDA- Object Counting (line)\nDDA- Object Counting (area)\nItem monitoring\nHeat Map\nFace Detection \nDDA2- Advanced Object Classification\nDDA- Audio Exception\nDDA- Illegal Parking Detection\nDDA- Loitering Detection","Yes","call for special offer",372]
[1,1,null,"DMA-340IPEN-28-V4",null,"Eye-Sight","Camera-H.265 Eye-Sight Series, Mini dome, IR 10M, 2.8mm Lens 4MP with PoE","4MP","Dome Anti-Vandal","True WDR","Fixed","2.8mm (93°)","IP67/\nIK10","10M","PR-B10BJB / PR-WB-A","Audio In \nAudio Out\nI/O\nSD Card\nBuilt-in Mic\nCheck Point Protect","Camera Tampering \nDDA- Line Crossing \nDDA- Sterile Area\nDDA- Object Counting (line)\nDDA- Object Counting (area)\nItem monitoring\nHeat Map\nFace Detection","Yes",null,290]
[1,1,null,"DAI-340IPEN-28-V4",null,"Eye-Sight","Camera-H.265 Eye-Sight Series, Anti-Vandal, IR 20M(3 LED Array), 2.8mm lens , 4M with PoE","4MP","Dome Anti-Vandal","True WDR","Fixed","2.8mm (93°)","IP67/\nIK10","20M","PR-JB12IP66 / PR-ICB21 / PR-WB-A","Audio In\nSD Card\nI/O\nBuilt-in Mic\nCheck Point Protect","Camera Tampering \nDDA- Line Crossing \nDDA- Sterile Area\nDDA- Object Counting (line)\nDDA- Object Counting (area)\nItem monitoring\nHeat Map\nFace Detection \nDDA2- Advanced Object Classification","Yes",null,301]
[1,1,null,"DAI-340IPEN-MVF-V4",null,"Eye-Sight","Camera-H.265 Eye-Sight Series, Anti-Vandal, IR 40M(2 LED Array), Motorized2.8-12mm lens, 4M with PoE","4MP","Dome Anti-Vandal","True WDR","Motorized Vari-Focal","2.8-12mm\n(98°-28°)","IP67/\nIK10","40M","PR-JB14IP66 / PR-ICB23","Audio In \nAudio Out\nI/O\nSD Card\nBuilt-in Mic\nCheck Point Protect","Camera Tampering \nDDA- Line Crossing \nDDA- Sterile Area\nDDA- Object Counting (line)\nDDA- Object Counting (area)\nItem monitoring\nHeat Map\nFace Detection\nDDA2- Advanced Object Classification","Yes",null,486]
[1,1,null,"DI-340IPEN-28-V4",null,"Eye-Sight","Camera- H.265 Eye-Sight Series,, Dome/Turret IR 20M(1 LED Array), 2.8mm Lens, 4M with PoE","4MP","Turret/Dome","True WDR","Fixed","2.8mm (96°)","IP67","20M","PR-DJB12IP66/\nPR-JB12IP66/\nPR-JB12IP64/ PR-WB-A","Audio In \nAudio Out\nSD Card\nBuilt-in Mic\nCheck Point Protect","Camera Tampering \nDDA- Line Crossing \nDDA- Sterile Area\nDDA- Object Counting (line)\nDDA- Object Counting (area)\nItem monitoring\nHeat Map\nFace Detection\nDDA2- Advanced Object Classification","Yes",null,269]
[1,1,null,"DI-340IPEN-28-G-V4",null,"Eye-Sight","Camera- H.265 Eye-Sight Series,, Dome/Turret IR 20M(1 LED Array), 2.8mm Lens, 4M with PoE","4MP","Turret/Dome","True WDR","Fixed","2.8mm (100°)","IP67","20M","PR-JB14IP66-G/\nPR-WB-A-G","Audio In \nAudio Out\nSD Card\nBuilt-in Mic\nCheck Point Protect","Camera Tampering \nDDA- Line Crossing \nDDA- Sterile Area\nDDA- Object Counting (line)\nDDA- Object Counting (area)\nItem monitoring\nHeat Map\nFace Detection \nDDA2- Advanced Object Classification","Yes",null,273]
[1,1,null,"DI-340IPEN-MVF-V4",null,"Eye-Sight","Camera- H.265 Eye-Sight Series, Dome/Turret IR 40M(2 LED Array), Motorized  2.8-12mm lens, 4M with P","4MP","Turret/Dome","True WDR","Motorized Vari-Focal","2.8-12mm  (100°-29°)","IP67","40M","PR-DJB14IP66/\nPR-JB14IP66/\nPR-JB14IP64/\nPR-WB-A","Audio In \nAudio Out\nI/O\nSD Card\nBuilt-in Mic\nCheck Point Protect","Camera Tampering \nDDA- Line Crossing \nDDA- Sterile Area\nDDA- Object Counting (line)\nDDA- Object Counting (area)\nItem monitoring\nHeat Map\nFace Detection \nDDA2- Advanced Object Classification","Yes",null,409]
[1,null,null,"DI-340IPEN-MVF-G-V4",null,"Eye-Sight","Camera- H.265 Eye-Sight Series, Dome/Turret IR 40M(2 LED Array), Motorized  2.8-12mm lens, 4M with P","4MP","Turret/Dome","True WDR","Motorized Vari-Focal","2.8-12mm  (100°-29°)","IP67","40M","PR-DJB14IP66/\nPR-JB14IP66/\nPR-JB14IP64/\nPR-WB-A","Audio In \nAudio Out\nI/O\nSD Card\nBuilt-in Mic\nCheck Point Protect","Camera Tampering \nDDA- Line Crossing \nDDA- Sterile Area\nDDA- Object Counting (line)\nDDA- Object Counting (area)\nItem monitoring\nHeat Map\nFace Detection \nDDA2- Advanced Object Classification","Yes",null,411]
[1,1,null,"I4-340IPEN-36-V4",null,"Eye-Sight","Camera- H.265 Eye-Sight Series, Bullet, IR 40M(2 LED Array), 3.6mm lens, 4M with PoE","4MP","Bullet","True WDR","Fixed","3.6mm (79°)","IP67","40M","PR-JB12IP66/\nPR-JB12IP64","Audio In\nAudio Out\nBuilt-in Mic\nSD Card\nCheck Point Protect","Camera Tampering \nDDA- Line Crossing \nDDA- Sterile Area\nDDA- Object Counting (line)\nDDA- Object Counting (area)\nItem monitoring\nHeat Map\nFace Detection \nDDA2- Advanced Object Classification","Yes",null,300]
[1,1,null,"I4-340IPEN-36-G",null,"Eye-Sight","Camera- H.265 Eye-Sight Series, Bullet, IR 40M(2 LED Array), 3.6mm lens, 4M with PoE,grey","4MP","Bullet","True WDR","Fixed","3.6mm (80.6°)","IP67","40M","PR-JB12IP66/\nPR-JB12IP64","Audio In\nSD Card","Camera Tampering \nDDA- Line Crossing \nDDA- Sterile Area\nDDA- Object Counting (line)\nDDA- Object Counting (area)\nItem monitoring\nHeat Map\nFace Detection \nDDA2- Advanced Object Classification\nDDA- Audio Exception\nDDA- Illegal Parking Detection\nDDA- Loitering Detection","Yes","call for special offer",306]
[1,1,null,"I4-340IPEN-MVF-V4",null,"Eye-Sight","Camera- H.265 Eye-Sight Series, Bullet, IR 40M(2 LED Array), Motorized 2.8-12mm lens, 4M with PoE","4MP","Bullet","True WDR","Motorized Vari-Focal","2.8-12mm\n(100°-29°)","IP67","40M","PR-JB12IP66/\nPR-JB12IP64","Audio In \nSD Card\nCheck Point Protect","Camera Tampering \nDDA- Line Crossing \nDDA- Sterile Area\nDDA- Object Counting (line)\nDDA- Object Counting (area)\nItem monitoring\nHeat Map\nFace Detection\nDDA2- Advanced Object Classification","Yes",null,405]
[1,1,null,"I6-340IPEN-MVF-V4",null,"Eye-Sight","Camera- H.265 Eye-Sight Series, Bullet, IR 60M(4 LED Array), Motorized 2.8-12mm lens, 4M with PoE","4MP","Bullet","True WDR","Motorized Vari-Focal","2.8-12mm\n(105°-33°)","IP67","60M","PR-JB14IP66/\nPR-JB14IP64","Audio In \nAudio Out\nI/O\nSD Card\nBuilt-in Mic\nCheck Point Protect","Camera Tampering \nDDA- Line Crossing \nDDA- Sterile Area\nDDA- Object Counting (line)\nDDA- Object Counting (area)\nItem monitoring\nHeat Map\nFace Detection\nDDA2- Advanced Object Classification","Yes",null,471]
[1,1,null,"I6-340IPEN-MVF-G-V4",null,"Eye-Sight","Camera- H.265 Eye-Sight Series, Bullet, IR 60M(4 LED Array), Motorized 2.8-12mm lens, 4M with PoE","4MP","Bullet","True WDR","Motorized Vari-Focal","2.8-12mm\n(96°-32°)","IP67","60M","PR-JB14IP66/\nPR-JB14IP64","Audio In\nAudio Out\nSD Card\nBuilt-in Mic\nI/O\nCheck Point Protect","Camera Tampering \nDDA- Line Crossing \nDDA- Sterile Area\nDDA- Object Counting (line)\nDDA- Object Counting (area)\nItem monitoring\nHeat Map\nFace Detection \nDDA2- Advanced Object Classification","Yes",null,485]
[1,1,null,"I8-340IPEN-MVF2-V4",null,"Eye-Sight","Camera- H.265 Eye-Sight Series, Bullet, IR 80M(4 LED Array), Motorized 7-22mm lens, 4M with PoE","4MP","Bullet","True WDR","Motorized Vari-Focal","7-22mm\n(43°-18°)","IP67","80M","PR-JB14IP66/\nPR-JB14IP64","Audio In\nAudio Out\nSD Card\nI/O\nCheck Point Protect","Camera Tampering \nDDA- Line Crossing \nDDA- Sterile Area\nDDA- Object Counting (line)\nDDA- Object Counting (area)\nItem monitoring\nHeat Map\nFace Detection \nDDA2- Advanced Object Classification","Yes",null,515]
[1,1,null,"DI-360IPEN-28-V4",null,"Eye-Sight","Camera-  Eye-Sight Series,, Dome/Turret IR 20M, 2.8mm Lens, Check Point embedded，6M with PoE","6MP","Turret/Dome","True WDR","Fixed","2.8mm (104°)","IP67","20M","PR-DJB12IP66/\nPR-JB12IP66/\nPR-JB12IP64/ PR-WB-A","Audio In \nAudio Out\nSD Card\nBuilt-in Mic\nCheck Point Protect","Camera Tampering \nDDA- Line Crossing \nDDA- Sterile Area\nDDA- Object Counting (line)\nDDA- Object Counting (area)\nItem monitoring\nHeat Map\nFace Detection \nDDA2- Advanced Object Classification\nDDA- Audio Exception\nDDA- Illegal Parking Detection\nDDA- Loitering Detection","Yes",null,320]
[1,1,null,"DI-360IPEN-MVF-V4",null,"Eye-Sight","Camera-  Eye-Sight Series, Dome/Turret IR 40M, Motorized  2.8-12mm lens,Check Point embedded, 6M wi","6MP","Turret/Dome","True WDR","Motorized Vari-Focal","2.8-12mm  (112°-35°)","IP67","40M","PR-DJB14IP66/\nPR-JB14IP66/\nPR-JB14IP64/\nPR-WB-A","Audio In \nAudio Out\nI/O\nSD Card\nBuilt-in Mic\nCheck Point Protect","Camera Tampering \nDDA- Line Crossing \nDDA- Sterile Area\nDDA- Object Counting (line)\nDDA- Object Counting (area)\nItem monitoring\nHeat Map\nFace Detection \nDDA2- Advanced Object Classification\nDDA- Audio Exception\nDDA- Illegal Parking Detection\nDDA- Loitering Detection","Yes",null,444]
[1,1,null,"DMA-360IPEN-28-V4",null,"Eye-Sight","Camera-H.265 Eye-Sight Series, Mini dome, IR 10M, 2.8mm Lens, CheckPoint embedded,6MP with PoE","6MP","Dome Anti-Vandal","True WDR","Fixed","2.8mm (100°)","IP67/\nIK10","10M","PR-B10BJB / PR-WB-A","Audio In \nAudio Out\nI/O\nSD Card\nBuilt-in Mic\nCheck Point Protect","Camera Tampering \nDDA- Line Crossing \nDDA- Sterile Area\nDDA- Object Counting (line)\nDDA- Object Counting (area)\nItem monitoring\nHeat Map\nFace Detection \nDDA2- Advanced Object Classification\nDDA- Audio Exception\nDDA- Illegal Parking Detection\nDDA- Loitering Detection","Yes",null,350]
[1,1,null,"I4-360IPEN-36-V4",null,"Eye-Sight","Camera-  Eye-Sight Series, Bullet, IR 40M, 3.6mm lens,checkPoint embedded, 6M with PoE","6MP","Bullet","True WDR","Fixed","3.6mm (78°)","IP67","40M","PR-JB12IP66/\nPR-JB12IP64","Audio In \nAudio Out\nI/O\nSD Card\nBuilt-in Mic\nCheck Point Protect","Camera Tampering \nDDA- Line Crossing \nDDA- Sterile Area\nDDA- Object Counting (line)\nDDA- Object Counting (area)\nItem monitoring\nHeat Map\nFace Detection \nDDA2- Advanced Object Classification\nDDA- Audio Exception\nDDA- Illegal Parking Detection\nDDA- Loitering Detection","Yes",null,348]
[1,1,null,"I4-360IPEN-MVF-V4",null,"Eye-Sight","Camera- Eye-Sight Series, Bullet, IR 40M, Motorized 2.8-12mm lens, Check Point embedded,6M with PoE","6MP","Bullet","True WDR","Motorized Vari-Focal","2.8-12mm  (108°-35°)","IP67","40M","PR-JB12IP66/\nPR-JB12IP64","Audio In \nAudio Out\nI/O\nSD Card\nBuilt-in Mic\nCheck Point Protect","Camera Tampering \nDDA- Line Crossing \nDDA- Sterile Area\nDDA- Object Counting (line)\nDDA- Object Counting (area)\nItem monitoring\nHeat Map\nFace Detection \nDDA2- Advanced Object Classification\nDDA- Audio Exception\nDDA- Illegal Parking Detection\nDDA- Loitering Detection","Yes",null,443]
[1,1,null,"I6-360IPEN-MVF-V4",null,"Eye-Sight","Camera- H.265 Eye-Sight Series, Bullet, IR 60M(4 LED Array), Motorized 2.8-12mm lens, 6M with PoE","6MP","Bullet","True WDR","Motorized Vari-Focal","2.8-12mm (108°-35°)","IP67","60M","PR-JB14IP66/\nPR-JB14IP64","Audio In \nAudio Out\nI/O\nSD Card\nBuilt-in Mic\nCheck Point Protect","Camera Tampering \nDDA- Line Crossing \nDDA- Sterile Area\nDDA- Object Counting (line)\nDDA- Object Counting (area)\nItem monitoring\nHeat Map\nFace Detection \nDDA2- Advanced Object Classification\nDDA- Audio Exception\nDDA- Illegal Parking Detection\nDDA- Loitering Detection","Yes",null,527]
[1,1,null,"DMA-380IPEN-28-V3",null,"Eye-Sight","Camera-H.265 Eye-Sight Series, Mini dome, IR 10M, 2.8mm Lens 8MP with PoE","8MP","Dome Anti-Vandal","True WDR","Fixed","2.8mm (103°)","IP66/\nIK10","10M","PR-B10BJB / PR-WB-A","Audio In \nAudio Out\nI/O\nSD Card\nBuilt-in Mic\nCheck Point Protect","Camera Tampering \nDDA- Line Crossing \nDDA- Sterile Area\nDDA- Object Counting (line)\nDDA- Object Counting (area)\nItem monitoring\nHeat Map\nFace Detection \nDDA2- Advanced Object Classification","Yes",null,432]
[1,1,null,"DI-380IPEN-MVF-V3",null,"Eye-Sight","Camera- H.265 Eye-Sight Series,Dome/Turret IR 40M(2 LED Array), Motorized 2.8-12mm lens, 8M with PoE","8MP","Turret/Dome","True WDR","Motorized Vari-Focal","2.8-12mm\n(96°-32°)","IP67","40M","PR-DJB14IP66/\nPR-JB14IP66/\nPR-JB14IP64/\nPR-WB-A","Audio In \nBuilt-in Mic\nSD Card\nCheck Point Protect","Camera Tampering \nDDA- Line Crossing \nDDA- Sterile Area\nDDA- Object Counting (line)\nDDA- Object Counting (area)\nItem monitoring\nHeat Map\nFace Detection \nDDA2- Advanced Object Classification\nDDA- Audio Exception\nDDA- Illegal Parking Detection\nDDA- Loitering Detection","Yes",null,588]
[1,1,null,"DI-380IPEN-MVF-G-V3",null,"Eye-Sight","Camera- H.265 Eye-Sight Series,Dome/Turret IR 40M(2 LED Array), Motorized 2.8-12mm lens, 8M with PoE","8MP","Turret/Dome","True WDR","Motorized Vari-Focal","2.8-12mm\n(96°-32°)","IP67","40M","PR-JB14IP66-G/\nPR-WB-A-G","Audio In \nBuilt-in Mic\nSD Card\nCheck Point Protect","Camera Tampering \nDDA- Line Crossing \nDDA- Sterile Area\nDDA- Object Counting (line)\nDDA- Object Counting (area)\nItem monitoring\nHeat Map\nFace Detection \nDDA2- Advanced Object Classification\nDDA- Audio Exception\nDDA- Illegal Parking Detection\nDDA- Loitering Detection","Yes",null,593]
[1,1,null,"DAI-380IPEN-MVF-V3",null,"Eye-Sight","Camera-H.265 Eye-Sight Series, Anti-Vandal, IR 40M(2 LED Array), Motorized2.8-12mm lens, 8M with PoE","8MP","Dome Anti-Vandal","True WDR","Motorized Vari-Focal","2.8-12mm\n(95°- 32°)","IP67/\nIK10","40M","PR-JB14IP66 / PR-ICB23","Audio In \nBuilt-in Mic \nAudio Out\nI/O\nSD Card\nCheck Point Protect","Camera Tampering \nDDA- Line Crossing \nDDA- Sterile Area\nDDA- Object Counting (line)\nDDA- Object Counting (area)\nItem monitoring\nHeat Map\nFace Detection \nDDA2- Advanced Object Classification\nDDA- Audio Exception\nDDA- Illegal Parking Detection\nDDA- Loitering Detection","Yes",null,605]
[1,1,null,"I6-380IPEN-MVF-V3",null,"Eye-Sight","Camera- H.265 Eye-Sight Series, Bullet, IR 60M(4 LED Array), Motorized 2.8-12mm lens, 8M with PoE","8MP","Bullet","True WDR","Motorized Vari-Focal","2.8-12mm\n(96°-32°)","IP67","60M","PR-JB14IP66/\nPR-JB14IP64","Audio In \nAudio Out\nI/O\nSD Card\nCheck Point Protect","Camera Tampering \nDDA- Line Crossing \nDDA- Sterile Area\nDDA- Object Counting (line)\nDDA- Object Counting (area)\nItem monitoring\nHeat Map\nFace Detection \nDDA2- Advanced Object Classification\nDDA- Audio Exception\nDDA- Illegal Parking Detection\nDDA- Loitering Detection","Yes",null,605]
[null,null,null,"DAI-2120IPEN-MVF-V5",null,"Eye-Sight","Camera-Eye-sight Series, CheckPoint embedded, Anti-Vandal, IR 40M,Motorized 2.8-12mm lens 12MwithPOE","8MP","Dome Anti-Vandal","True WDR","Motorized Vari-Focal","2.8-12mm\n(98°-47°)","IP67/\nIK10","40M","PR-JB14IP66 / PR-ICB23","Audio In \nBuilt-in Mic \nAudio Out\nI/O\nSD Card\nCheck Point Protect","Camera Tampering \nDDA- Line Crossing \nDDA- Sterile Area\nDDA- Object Counting (line)\nDDA- Object Counting (area)\nItem monitoring\nHeat Map\nFace Detection \nDDA2- Advanced Object Classification\nDDA- Audio Exception\nDDA- Illegal Parking Detection\nDDA- Loitering Detection","Yes","New Model",972.9]
[1,null,null,"I6-2120IPEN-MVF-V5",null,"Eye-Sight","Camera- Eye-Sight Series,CheckPonit Bullet, IR 60M, Motorized 2.8-12mm lens, 12M with PoE","12MP","Bullet","True WDR","Motorized Vari-Focal","2.8-12mm\n(96°-47°)","IP67","60M","PR-JB14IP66/\nPR-JB14IP64","Audio In\nBuilt-in Mic\nAudio Out\nI/O\nSD Card\nCheck Point Protect","Camera Tampering \nDDA- Line Crossing \nDDA- Sterile Area\nDDA- Object Counting (line)\nDDA- Object Counting (area)\nItem monitoring\nHeat Map\nFace Detection \nDDA2- Advanced Object Classification\nDDA- Audio Exception\nDDA- Illegal Parking Detection\nDDA- Loitering Detection","Yes",null,972.9]
[1,1,null,"I6-320LPR-MVF1",null,"Smart-Sight","Camera-Smart series ,LPR, Bullet, 2MP IR 40M(2LED Array), 2.8-12mm MVF Lens, with POE","2MP","Bullet","True WDR","Motorized Vari-Focal","2.8-12mm\n(103.4°-32.4°)","IP67","60M","PR-JB14IP66/\nPR-JB14IP64","Audio In\nAudio Out\nSD Card\nI/O","LPR","No",null,1000]
[1,1,null,"I6-320LPR-MVF2",null,"Smart-Sight","Camera-Smart series ,LPR, Bullet, 2MP IR 40M(2LED Array), 7-22mm MVF Lens, with POE","2MP","Bullet","True WDR","Motorized Vari-Focal","7-22mm\n(44°-17.6°)","IP67","60M","PR-JB14IP66/\nPR-JB14IP64","Audio In\nAudio Out\nSD Card\nI/O","LPR","No",null,1000]
[1,1,null,"I6-340LPRN-MVF1",null,"Smart-Sight","Camera-Smart series, LPR, Bullet, 4MP IR 40M(2LED Array),2.8-12mm MVF Lens, with POE,support Wiegand","4MP","Bullet","True WDR","Motorized Vari-Focal","2.8-12mm\n(103°-48°)","IP67","60M","PR-JB14IP66/\nPR-JB14IP64","Audio In\nAudio Out\nSD Card\nI/O\nWigand","LPR","Yes","EOL, replace by I6-240LPRN-MVF1",1179]
[1,null,null,"I6-240LPRN-MVF1",null,"Smart-Sight","Camera-Smart series, LPR, Bullet, 4MP IR 40M(2LED Array),2.8-12mm MVF Lens, with POE,support Wiegand","4MP","Bullet","True WDR","Motorized Vari-Focal","2.8-12mm\n(110°-48°)","IP67","60M","PR-JB14IP66/\nPR-JB14IP64","Audio In\nAudio Out\nSD Card\nI/O\nWigand","LPR","Yes","New Model",1200]
[1,null,null,"I6-240LPRN-MVF2",null,"Smart-Sight","Camera-Smart series, LPR, Bullet, 4MP IR 40M(2LED Array),8-32mm MVF Lens, with POE,support Wiegand","4MP","Bullet","True WDR","Motorized Vari-Focal","8-32mm\n(42°-16°)","IP67","60M","PR-JB14IP66/\nPR-JB14IP64","Audio In\nAudio Out\nSD Card\nI/O\nWigand","LPR","Yes",null,1270]
[1,1,null,"DH-340ADN-MVF-V4",null,"Smart-Sight","Camera- H.265 Smart-Sight  Smart alert Series,, Dome/Turret, IR LED, motorized Lens 4M withPoE","4MP","Turret/Dome","True WDR","Motorized Vari-Focal","2.8-12mm  (95°-32°)","IP67","40M","PR-DJB14IP66/\nPR-JB14IP66/\nPR-JB14IP64/\nPR-WB-A","Audio In\nAudio Out \nBuilt-in Mic \nBuilt-in speaker\nI/O\nRed/Blue Strobe Light\nSD Card\nColor at night\nCheck Point Protect","DDA- Line Crossing \nDDA- Sterile Area\nActive Deterrence","Yes",null,430]
[null,null,null,"DH-340ADN-MVF-G-V4",null,"Smart-Sight","Camera- H.265 Smart-Sight  Smart alert Series,, Dome/Turret, IR LED, motorized Lens 4M withPoE","4MP","Turret/Dome","True WDR","Motorized Vari-Focal","2.8-12mm  (95°-32°)","IP67","40M","PR-DJB14IP66/\nPR-JB14IP66/\nPR-JB14IP64/\nPR-WB-A","Audio In\nAudio Out \nBuilt-in Mic \nBuilt-in speaker\nI/O\nRed/Blue Strobe Light\nSD Card\nColor at night\nCheck Point Protect","DDA- Line Crossing \nDDA- Sterile Area\nActive Deterrence","Yes",null,435]
[1,1,null,"I4-340AD-MVF",null,"Smart-Sight","Camera- H.265 S-Sight  active deterrence Series, Bullet IR LED, motorized Lens 4M with PoE","4MP","Bullet","True WDR","Motorized Vari-Focal","2.8-12mm\n(94.2°-29.8°)","IP67","40M","PR-JB12IP66/\nPR-JB12IP64","Audio In \nBuilt-in Mic \n Built-in speaker\nI/O\nRed/Blue Strobe Light\nSD Card","DDA- Line Crossing \nDDA- Sterile Area\nActive Deterrence","No","Price drop",425]
[1,1,null,"BMH-340ADN-MVF-V4",null,"Smart-Sight","Camera- H.265 Smart-Sight smart alert Series, Bullet IR LED, motorized Lens 4M with PoE","4MP","Bullet","True WDR","Motorized Vari-Focal","2.8-12mm \n (97-32°)","IP67","40M","PR-JB12IP66/\nPR-JB12IP64","Audio In\nAudio Out \nBuilt-in Mic \nBuilt-in speaker\nI/O\nRed/Blue Strobe Light\nSD Card\nColor at night\nCheck Point Protect","DDA- Line Crossing \nDDA- Sterile Area\nActive Deterrence","Yes",null,459]
[1,null,null,"DPAN2-340ADRN",null,"Smart-Sight","Camera-H.265 , panaromic, white LED, 180° lens, 2*4mp stich 8Mp with POE","8MP","Panoramic","DWDR","Fixed","2x 3.5mm (180°)","IP67/IK10","20M","None","Audio In\nAudio Out \nBuilt-in Mic \nBuilt-in speaker\nI/O\nSD Card\nColor at night","Camera Tampering \nStandard- Line Crossing \nStandard- Sterile Area\nDDA- Line Crossing \nDDA- Sterile Area\nActive Deterrence","Yes","New Model",748]
[1,1,null,"FEI-360IPN-V3",null,"Special","Camera-H.265 IP Series,fisheye,6Mega-Pixel with PoE","6MP","Fish-Eye","DWDR","Fish-Eye","1.65mm","IP67/IK10","15M","PR-B50JB","Audio In\nAudio Out\nSD Card\nI/O\nBuilt-in Mic","Camera Tampering \nDDA- Line Crossing \nDDA- Sterile Area\nDDA- Object Counting (line)\nDDA- Object Counting (area)\nHeat Map","Yes",null,630]
[1,null,null,"FEI-2120IPN",null,"Special","Camera-H.265 IP Series,fisheye,12Mega-Pixel with PoE","12MP","Fish-Eye","DWDR","Fish-Eye","1.65mm","IP67/IK10","15M","PR-B50JB","Audio In\nAudio Out\nSD Card\nI/O\nBuilt-in Mic","Camera Tampering \nDDA- Line Crossing \nDDA- Sterile Area\nDDA- Object Counting (line)\nDDA- Object Counting (area)\nHeat Map","Yes",null,950]
[1,1,null,"IV-320IPSN-37",null,"Special","Camera-H.265 , Dummy PIR, IR 10M(24 LEDs), 3.7mm Pinhole Lens , 1080P PoE","2MP","Hidden","DWDR","Fixed","3.7mm (83°)","IP67","10M","None","Audio In\nSD Card\nBuilt-in Mic","Camera Tampering  \nStandard- Line Crossing \nStandard- Sterile Area","Yes",null,190]
[1,null,null,"DH-THERMAL-3-V2",null,"Special","Thermal Network Dome Camera, 5MP,3.2mm thermal lens","5MP","Turret/Dome","True WDR","Fixed","Thermal:\n3mm  (53°)\n\nOptical:\n4mm  (74°)","IP66","20M","PR-DJB12IP66/\nPR-JB12IP66/\nPR-JB12IP64/ PR-WB-A","Audio In\nSD Card\nI/O\nBuilt-in Speaker\nBuilt-in Mic \nCheck Point Protect\n","Fire Detection\nTemperture alert\nCamera Tampering \nDDA- Line Crossing \nDDA- Sterile Area\nDDA- Object Counting (line)\nDDA- Object Counting (area)\nItem monitoring\nHeat Map\nFace Detection \nDDA- Audio Exception\nDDA- Illegal Parking Detection\nDDA- Loitering Detection","Yes",null,1390]
[1,null,null,"DH-THERMAL-7-V2",null,"Special","Thermal Network Dome Camera, 5MP,7 mm thermal lens","5MP","Turret/Dome","True WDR","Fixed","Thermal:\n7mm  (25°)\n\nOptical:\n8mm  (35°)","IP66","20M","PR-DJB12IP66/\nPR-JB12IP66/\nPR-JB12IP64/ PR-WB-A","Audio In\nSD Card\nI/O\nBuilt-in Speaker\nBuilt-in Mic \nCheck Point Protect\n","Fire Detection\nTemperture alert\nCamera Tampering \nDDA- Line Crossing \nDDA- Sterile Area\nDDA- Object Counting (line)\nDDA- Object Counting (area)\nItem monitoring\nHeat Map\nFace Detection \nDDA- Audio Exception\nDDA- Illegal Parking Detection\nDDA- Loitering Detection","Yes",null,1390]
[1,1,null,"BMH-THERMAL-3-V2",null,"Special","Thermal Network Bullet Camera, 5MP,3.2mm thermal lens","5MP","Bullet","True WDR","Fixed","Thermal:\n3mm  (53°)\n\nOptical:\n4mm  (74°)","IP66","20M","PR-JB12IP66/\nPR-JB12IP64","Audio In\nSD Card\nI/O\nBuilt-in Speaker\nCheck Point Protect\n","Fire Detection\nTemperture alert\nCamera Tampering \nDDA- Line Crossing \nDDA- Sterile Area\nDDA- Object Counting (line)\nDDA- Object Counting (area)\nItem monitoring\nHeat Map\nFace Detection \nDDA- Audio Exception\nDDA- Illegal Parking Detection\nDDA- Loitering Detection","Yes",null,1226]
[1,1,null,"BMH-THERMAL-7-V2",null,"Special","Thermal Network Bullet Camera, 5MP,7 mm thermal lens","5MP","Bullet","True WDR","Fixed","Thermal:\n7mm  (25°)\n\nOptical:\n8mm  (35°)","IP66","20M","PR-JB12IP66/\nPR-JB12IP64","Audio In\nSD Card\nI/O\nBuilt-in Speaker\nCheck Point Protect\n","Fire Detection\nTemperture alert\nCamera Tampering \nDDA- Line Crossing \nDDA- Sterile Area\nDDA- Object Counting (line)\nDDA- Object Counting (area)\nItem monitoring\nHeat Map\nFace Detection \nDDA- Audio Exception\nDDA- Illegal Parking Detection\nDDA- Loitering Detection","Yes",null,1245]
[1,1,null,"BLH-THERMAL-19",null,"Special","Thermal Network Bullet Camera, 5MP,19mm thermal lens","5MP","Bullet","True WDR","Fixed","Thermal: \n19mm (19.5°)\n\nOptical:\n12mm (26.6°)\n","IP66","85M","PR-JB12IP66/\nPR-JB12IP64","Audio In\nSD Card\nI/O\nBuilt-in Speaker\n","Fire Detection\nTemperture alert\nCamera Tampering \nDDA- Line Crossing \nDDA- Sterile Area\nDDA- Object Counting (line)\nDDA- Object Counting (area)\nItem monitoring\nHeat Map\nFace Detection \nDDA- Audio Exception\nDDA- Illegal Parking Detection\nDDA- Loitering Detection","Yes",null,3999.24]
[1,1,null,"BLH-THERMAL-25",null,"Special","Thermal Network Bullet Camera, 5MP,25mm thermal lens","5MP","Bullet","True WDR","Fixed","Thermal: 25mm (15°)\n\nOptical:\n16mm (19.8°)\n","IP66","85M","PR-JB12IP66/\nPR-JB12IP64","Audio In\nSD Card\nI/O\nBuilt-in Speaker\n","Fire Detection\nTemperture alert\nCamera Tampering \nDDA- Line Crossing \nDDA- Sterile Area\nDDA- Object Counting (line)\nDDA- Object Counting (area)\nItem monitoring\nHeat Map\nFace Detection \nDDA- Audio Exception\nDDA- Illegal Parking Detection\nDDA- Loitering Detection","Yes",null,4890]
[1,1,null,"DB-320WIPN",null,"Special","Video doorbell camera, 2MP.2.3mm Lens,Access control function","2MP","DoorBell","DWDR","Fixed","2.3mm  (139°) ","IP65","10M","None","Built-in Mic\nBuilt-in Speaker\nI/O\nSD Card\nWigand\nWi-Fi","SMD\nFace Detection","Yes",null,355]
[1,1,null,"DV-320SRN-36",null,"Rainbow","Camera- H.265 S-Sight  Rainbow Series,, Dome/Turret, White LED, 3.6mm Lens 2M with PoE","2MP","Turret/Dome","True WDR","Fixed","3.6mm (84.6°)","IP67","25M (White Led)","PR-DJB12IP66/\nPR-JB12IP66/\nPR-JB12IP64/ PR-WB-A","Built-in Mic\nSD Card\nColor at night","Camera Tampering \nDDA- Line Crossing \nDDA- Sterile Area\nDDA- Object Counting","Yes","call for special offer",198]
[1,1,null,"DV-320SRN-28",null,"Rainbow","Camera- H.265 S-Sight  Rainbow Series,, Dome/Turret, White LED, 2.8mm Lens 2M with PoE","2MP","Turret/Dome","True WDR","Fixed","2.8mm (105.2°)","IP67","25M (White Led)","PR-DJB12IP66/\nPR-JB12IP66/\nPR-JB12IP64/ PR-WB-A","Built-in Mic\nSD Card\nColor at night","Camera Tampering \nDDA- Line Crossing \nDDA- Sterile Area\nDDA- Object Counting","Yes","call for special offer",196]
[1,1,null,"DH-320SRN-MVF",null,"Rainbow","Camera- H.265 S-Sight Series, Dome/Turret IR 40M(2 LED Array), Motorized  2.8-12mm lens, 2M with PoE","2MP","Turret/Dome","True WDR","Motorized Vari-Focal","2.8-12mm\n(105.4°-34°)","IP67","40M Hybrid High Power LED","PR-DJB14IP66/\nPR-JB14IP66/\nPR-JB14IP64/\nPR-WB-A","Audio In \nBuilt-in Mic\nSD Card\nColor at night","Camera Tampering \nDDA- Line Crossing \nDDA- Sterile Area\nDDA- Object Counting","Yes","call for special offer",297]
[1,1,null,"TL-320IPSR-36",null,"Rainbow","Camera- H.265 S-Sight Rainbow Series, bullet,  White LED, 3.6mm Lens 2M with PoE","2MP","Bullet","DWDR","Fixed","3.6mm (84.8°)","IP67","25M (White Led)","PR-JB12IP66/\nPR-JB12IP64/ PR-WB-A","Built-in Mic \nSD Card\nColor at night","Camera Tampering \nStandard- Line Crossing \nStandard- Sterile Area","No","call for special offer",196]
[1,1,null,"BSV-320SRN-36",null,"Rainbow","Camera- H.265 S-Sight Rainbow Series, bullet,  White LED, 3.6mm Lens 2M with PoE","2MP","Bullet","True WDR","Fixed","3.6mm (84.6°)","IP67","25M (White Led)","PR-JB12IP66/\nPR-JB12IP64","Built-in Mic\nSD Card\nColor at night","Camera Tampering \nDDA- Line Crossing \nDDA- Sterile Area\nDDA- Object Counting","Yes","call for special offer",196]
[1,1,null,"BMV-320SRN-36",null,"Rainbow","Camera- H.265 S-Sight  Rainbow Series,, bullet, White LED, 3.6mm Lens 2M with PoE","2MP","Bullet","True WDR","Fixed","3.6mm (84.6°)","IP67","40M (White Led)","PR-JB12IP66/\nPR-JB12IP64","Audio In \nBuilt-in Mic\nSD Card\nColor at night","Camera Tampering \nDDA- Line Crossing \nDDA- Sterile Area\nDDA- Object Counting","Yes","call for special offer",220]
[1,1,null,"BMH-320SRN-MVF",null,"Rainbow","Camera- H.265 S-Sight Series, Bullet, IR 40M(2 LED Array), Motorized 2.8-12mm lens, 2M with PoE","2MP","Bullet","True WDR","Motorized Vari-Focal","2.8-12mm\n(105.4°-34°)","IP67","40M Hybrid High Power LED","PR-JB12IP66/\nPR-JB12IP64","Audio In \nBuilt-in Mic\nSD Card\nColor at night","Camera Tampering \nDDA- Line Crossing \nDDA- Sterile Area\nDDA- Object Counting","Yes",null,293.75784000000004]
[1,1,null,"DV-340SRN-28",null,"Rainbow","Camera- H.265 S-Sight  Rainbow Series,, Dome/Turret, White LED, 2.8mm Lens 4M with PoE","4MP","Turret/Dome","True WDR","Fixed","2.8mm (99°)","IP67","25M (White Led)","PR-DJB12IP66/\nPR-JB12IP66/\nPR-JB12IP64/ PR-WB-A","Audio In \nBuilt-in Mic\nSD Card\nColor at night","Camera Tampering \nDDA- Line Crossing \nDDA- Sterile Area\nDDA- Object Counting","Yes",null,210]
[1,1,null,"DH-340SRN-MVF",null,"Rainbow","Camera- H.265 S-Sight Series, Dome/Turret IR 40M(2 LED Array), Motorized  2.8-12mm lens, 4M with PoE","4MP","Turret/Dome","True WDR","Motorized Vari-Focal","2.8-12mm\n(105.4°-34°)","IP67","40M Hybrid High Power LED","PR-DJB14IP66/\nPR-JB14IP66/\nPR-JB14IP64/\nPR-WB-A","Audio In \nBuilt-in Mic\nSD Card\nColor at night","Camera Tampering \nDDA- Line Crossing \nDDA- Sterile Area\nDDA- Object Counting","Yes",null,319]
[1,1,null,"BSV-340SRN-36",null,"Rainbow","Camera- H.265 S-Sight Rainbow Series, bullet,  White LED, 3.6mm Lens 4M with PoE","4MP","Bullet","True WDR","Fixed","3.6mm (98°)","IP67","25M (White Led)","PR-JB12IP66/ PR-JB12IP64","Audio In \nSD Card\nColor at night","Camera Tampering \nDDA- Line Crossing \nDDA- Sterile Area\nDDA- Object Counting","Yes",null,213]
[1,1,null,"BMV-340SRN-36",null,"Rainbow","Camera- H.265 S-Sight  Rainbow Series,, bullet, White LED, 3.6mm Lens 4M with PoE","4MP","Bullet","True WDR","Fixed","3.6mm (79°)","IP67","40M (White Led)","PR-JB12IP66/ PR-JB12IP64","Audio In \nBuilt-in Mic\nSD Card\nColor at night","Camera Tampering \nDDA- Line Crossing \nDDA- Sterile Area\nDDA- Object Counting","Yes",null,244]
[1,1,null,"BMH-340SRN-MVF",null,"Rainbow","Camera- H.265 S-Sight Series, Bullet, IR 40M(2 LED Array), Motorized 2.8-12mm lens, 4M with PoE","4MP","Bullet","True WDR","Motorized Vari-Focal","2.8-12mm\n(97°-33°)","IP67","40M Hybrid High Power LED","PR-JB12IP66/ PR-JB12IP64","Audio In \nBuilt-in Mic\nSD Card\nColor at night","Camera Tampering \nDDA- Line Crossing \nDDA- Sterile Area\nDDA- Object Counting","Yes",null,320]
[1,1,null,"DL-340IPERN-36",null,"Rainbow","Camera- H.265 E-Sight Rainbow Series, Dome/Turret , White LED, 3.6mm Lens, 4M with PoE","4MP","Turret/Dome","True WDR","Fixed","3.6mm (77.9°)","IP67","25M (White Led)","PR-JB12IP66/\nPR-JB12IP64/ PR-WB-A","Audio In \nBuilt-in Mic\nSD Card\nColor at night","Camera Tampering \nDDA- Line Crossing \nDDA- Sterile Area\nDDA- Object Counting\nFace Detection \n","Yes","call for special offer",280]
[1,1,null,"TL-340IPERN-36",null,"Rainbow","Camera- H.265 E-Sight Rainbow Series, bullet, White LED, 3.6mm Lens, 4M with PoE","4MP","Bullet","True WDR","Fixed","3.6mm (77.9°)","IP67","25M (White Led)","PR-JB12IP66/\nPR-JB12IP64","Audio In \nBuilt-in Mic\nSD Card\nColor at night","Camera Tampering \nDDA- Line Crossing \nDDA- Sterile Area\nDDA- Object Counting\nFace Detection \n","Yes","call for special offer",290]

{"sheet":"DVR","index":3,"n_rows":17,"n_cols":18,"rows_kept":17,"cut":false,"hidden":false,"merged":[[0,3,0,16],[1,3,1,14],[1,15,1,16],[2,2,2,16]]}
[null,null,"DVR"]
[]
[]
[null,null,"Model","Free text","Description","No. of Channels","No. of IP Channels","HD Max Resolution","HD Max Real-Time Resolution","IP Max Resolution","Bandwidth","HDD","E-Sata","Audio","Video Output","Dry Contact","NDAA","PVP 2025"]
[null,null,"SH-4100A5N-2L(MM)-V2",null,"All In 1 Hybrid Stand Alone DVR-H.265 1080P Lite , 4CH Video Inputs. MM case",4,"up to 2","2MP Lite","2MP Lite","3MP","10Mbps/ 30Mbps","1 of 6TB max",0,"IN- 1+IPC Out- 1+IPC"," HDMI, VGA, ","Based on IPC Only","Yes",120]
[null,null,"SH-4050A5N-5L(MM)-V2",null,"H.265 All In 1 Hybrid NDAA DVR-5MP Lite, 4CH Video Inputs. MM case, CheckPoint Embedded, SMD",4,"up to 2","5MP Lite","2MP Lite","5MP","16Mbps/ 40Mbps","1 of 10TB max",0,"IN- 1+IPC Out- 1+IPC"," HDMI, VGA, CVBS","Based on IPC Only","Yes",185]
[null,null,"SH-4050A5N-8L(MM)-V2",null,"H.265 All In 1 Hybrid Stand Alone DVR-8MP Lite, 4CH Video Inputs. MM case",4,"up to 2","8MP Lite","4MP Lite","8MP","16Mbps/\n40Mbps","1 of 6TB max",0,"IN- 1+IPC Out- 1+IPC"," HDMI (4K), VGA, CVBS","Based on IPC Only","Yes",299]
[1,1,"SH-8100A5N-2L(MM)-V2",null,"All In 1 Hybrid Stand Alone DVR-H.265 1080P Lite , 8CH Video Inputs. MM case",8,"up to 4","2MP Lite","1MP ","5MP","16Mbps/\n60Mbps","1 of 6TB max",0,"IN- 1+IPC Out- 1+IPC"," HDMI, VGA","Based on IPC Only","Yes",160]
[null,null,"SH-8100A5N-5L(MM)-V2",null,"DVR-5MP Lite, 8CH Video Inputs, NDAA, CheckPoint Embedded, MM case. SMD",8,"up to 4","5MP Lite","2MP Lite","5MP","32Mbps/\n60Mbps","1 of 10TB max","32Mbps/\n60Mbps","IN- 1+IPC Out- 1+IPC"," HDMI, VGA, CVBS","Based on IPC Only","Yes",290]
[null,null,"SH-8100A5N-5L-V2",null,"DVR-5MP Lite, 8CH Video Inputs, NDAA, CheckPoint Embedded, Small 1U case",8,"up to 12","5MP Lite","2MP Lite","5MP","60Mbps/\n60Mbps","1 of 8TB max",1,"IN- 8+IPC Out- 1+IPC"," HDMI, VGA, CVBS","IN- 8+IPC Out- 2+IPC","Yes",368]
[null,null,"SH-8100A5N-8L(MM)-V2",null,"H.265 All In 1 Hybrid Stand Alone DVR-8MP Lite, 8CH Video Inputs. MM case",8,"up to 8","8MP Lite","4MP Lite","8MP","32Mbps/\n80Mbps","1 of 6TB max",0,"IN- 1+IPC Out- 1+IPC"," HDMI (4K), VGA, CVBS","Based on IPC Only","Yes",470]
[null,null,"SH-8100A5N-8L(1U)-V2",null,"H.265 All In 1 Hybrid Stand Alone DVR-8MP Lite, 8CH Video Inputs. 1U case",8,"up to 8","8MP Lite","4MP Lite","8MP","32Mbps/\n96Mbps","2 of 8TB max",1,"IN- 8+IPC Out- 1+IPC"," HDMI (4K), VGA, CVBS","IN- 8+IPC Out- 2+IPC","Yes",652]
[null,null,"SH-16200A5N-2L(MM)-V2",null,"All In 1 Hybrid Stand Alone DVR-H.265 1080P Lite , 16CH Video Inputs. MM case",16,"up to 18","2MP Lite","1MP","5MP","16Mbps/\n80Mbps","1 of 6TB max",0,"IN- 1+IPC Out- 1+IPC"," HDMI (4K), VGA, CVBS","Based on IPC Only","Yes",277]
[null,null,"SH-16200A5N-5L(MM)-V2",null,"H.265 All In 1 Hybrid Stand Alone DVR-5MP Lite, 16CH Video Inputs. MM case",16,"up to 16","5MP Lite","2MP Lite","5MP","32Mbps/\n80Mbps","1 of 6TB max",0,"IN- 1+IPC Out- 1+IPC"," HDMI, VGA, CVBS","Based on IPC Only","Yes",500]
[null,null,"SH-16200A5N-5L(1U)-V2",null,"H.265 All In 1 Hybrid Stand Alone DVR-5MP Lite, 16CH Video Inputs. 1U case",16,"up to 8","5MP Lite","2MP Lite","5MP","64Mbps/\n96Mbps","2 of 8TB max",1,"IN- 8+IPC Out- 1+IPC"," HDMI, VGA, CVBS","IN- 16+IPC Out- 4+IPC","Yes",644]
[null,null,"SH-16200A5N-8L(1U)-V2",null,"H.265 All In 1 Hybrid Stand Alone DVR- 8MP Lite, 16CH Video Inputs. 1U case",16,"up to 16","8MP Lite","4MP Lite","8MP","64Mbps/\n96Mbps","2 of 8TB max",1,"IN- 8+IPC Out- 1"," HDMI (4K), VGA,CVBS","IN- 16+IPC Out- 4+IPC","Yes",1290]
[null,null,"SH-32400A5N-5L(1.5U)-V2",null,"DVR-5MP Lite, 32CH Video Inputs, NDAA, CheckPoint Embedded,1.5U case.",32,"up to 16","5MP Lite","2MP Lite","5MP","88Mbps/\n160Mbps","4 of 8TB max",1,"IN- 16+IPC Out- 1+IPC"," HDMI, VGA, CVBS","IN- 16+IPC Out- 4+IPC","Yes",1550]

{"sheet":"HDC","index":4,"n_rows":51,"n_cols":16,"rows_kept":51,"cut":false,"hidden":false,"merged":[[0,3,0,14],[1,3,1,11],[1,12,1,14],[2,2,2,14]]}
[null,null,"HDC"]
[]
[]
[null,null,"Series","Free text","Series","Description","Resolution","Housing","Lens Type","Lens Focal","Protection","IR Range","Juntion box","Special features","Remarks","PVP 2025"]
[1,null,"DI-320AB-28",null,"Basic","Camera HD-2MP Basic series, Turret, IR 20M (1 LED Array), 2.8mm Lens","2MP","Turret/Dome","Fixed","2.8mm\n(88°)","IP67","20M","PR-JB12IP66 / PR-JB12IP64 / PR-WB-A","HLC",null,52.7]
[1,null,"I2-320AB-28",null,"Basic","Camera HD-2MP Basic series, Bullet, IR 20M (1 LED Array), 2.8mm Lens","2MP","Bullet","Fixed","2.8mm\n(88°)","IP67","20M","PR-JB12IP66 / PR-JB12IP64","None",null,52.7]
[1,null,"DI-33K0AB-28",null,"Basic","Camera HD-3K Basic series, Turret, IR 20M (1 LED Array), 2.8mm Lens","3K","Turret/Dome","Fixed","2.8mm\n(98°)","IP67","20M","PR-JB12IP66 / PR-JB12IP64 / PR-WB-A","Built-in Mic\nD-WDR\nHLC","EOL, replace with \nDH-33K0AB-28",80]
[null,null,"DH-33K0AB-28",null,"Basic","Camera HD-3K Basic series,Hybrid light,Turret, IR 20M , 2.8mm Lens","3K","Turret/Dome","Fixed","2.8mm\n(98°)","IP67","20M","PR-JB12IP66 / PR-JB12IP64 / PR-WB-A","Color at night\nBuilt-in Mic\nD-WDR","New model",80]
[null,null,"BSH-33K0AB-28",null,"Basic","Camera HD-3K Basic series, Hybrid light, Bullet, IR 20M , 2.8mm Lens","3K","Bullet","Fixed","2.8mm\n(98°)","IP67","20M","PR-JB12IP66 / PR-JB12IP64","Color at night\nBuilt-in Mic\nD-WDR",null,80]
[1,null,"DI-320A-28",null,"Pro","Camera HD- 2MP Pro series,  Dome/Turret IR 20M (1 LED Array), 2.8mm Lens","2MP","Turret/Dome","Fixed","2.8mm\n(88°)","IP67","20M","PR-JB12IP66 / PR-JB12IP64 / PR-WB-A","None",null,68]
[1,null,"DI-320A-VF",null,"Pro","Camera HD- 2MP Pro series,  Dome/Turret IR 40M(3LED Array), 2.8-12mm Lens","2MP","Turret/Dome","Vari-Focal","2.8-12mm\n(88°-33°)","IP67","40M","PR-JB14IP66 / PR-JB14IP64 / PR-WB-A","None",null,105]
[1,null,"DI-320A-VF-G",null,"Pro","Camera HD- 2MP Pro series, Turret IR 40M(3LED Array), 2.8-12mm Lens Grey","2MP","Turret/Dome","Vari-Focal","2.8-12mm\n(88°-33°)","IP67","40M","PR-JB14IP66-G/\nPR-WB-A-G","None",null,108]
[1,null,"I2-320A-28  ",null,"Pro","Camera HD- 2MP Pro series, Bullet, IR 20M (1 LED Array), 2.8mm Lens","2MP","Bullet","Fixed","2.8mm\n(88°)","IP67","20M","PR-JB12IP66 / PR-JB12IP64","None",null,69]
[1,null,"I4-320A-28",null,"Pro","Camera HD- 2MP Pro series, Bullet, IR 30M (2LED Array), 2.8mm Lens","2MP","Bullet","Fixed","2.8mm\n(88°)","IP67","40M","PR-JB12IP66 / PR-JB12IP64","None",null,85]
[1,null,"I4-320A-VF",null,"Pro","Camera HD- 2MP Pro series, Bullet, IR 40M (3 LED Array), 2.8-12mm Lens","2MP","Bullet","Vari-Focal","2.8-12mm\n(88°-33°)","IP67","40M","PR-JB12IP66 / PR-JB12IP64","None",null,108]
[1,null,"I4-320A-VF-G",null,"Pro","Camera HD- 2MP Pro series, Bullet, IR 40M (3 LED Array), 2.8-12mm Lens, Grey","2MP","Bullet","Vari-Focal","2.8-12mm\n(88°-33°)","IP67","40M","PR-JB12IP66-G","None","call for special offer",108]
[1,null,"DI-350A-28",null,"Pro","Camera HD- 5MP Pro series,  Dome/Turret IR 20M (1 LED Array), 2.8mm Lens","5MP","Turret/Dome","Fixed","2.8mm\n(91°)","IP67","20M","PR-JB12IP66 / PR-JB12IP64 / PR-WB-A","D-WDR","call for special offer",53.16]
[1,null,"DI-33K0AP-28",null,"Pro","Camera HD-3K Basic series, Turret, IR 20M (1 LED Array), 2.8mm Lens","3K","Turret/Dome","Fixed","2.8mm\n(100°)","IP67","20M","PR-JB12IP66 / PR-JB12IP64 / PR-WB-A","Built-in Mic \nD-WDR",null,99]
[1,null,"DI-350A-VF",null,"Pro","Camera HD- 5MP Pro Series,  Dome/Turret IR 40M(3 LED Array), 2.8-12mm lens","5MP","Turret/Dome","Vari-Focal","2.8-12mm\n(84°-32°)","IP67","40M","PR-JB14IP66 / PR-JB14IP64 / PR-WB-A","D-WDR","call for special offer",149]
[1,null,"DI-350A-MVF",null,"Pro","Camera HD- 5MP Pro Series,  Dome/Turret IR 40M(3 LED Array), Motorized  2.8-12mm lens","5MP","Turret/Dome","Motorized Vari-Focal","2.8-12mm\n(84°-32°)","IP67","40M","PR-JB14IP66 / PR-JB14IP64 / PR-WB-A","D-WDR","call for special offer",158]
[1,null,"DI-33K0AP-MVF",null,"Pro","Camera HD- 3K Pro Series, 16:9,DWDR,Audio over coax,Turret IR 40M, Motorized  2.8-12mm lens","3K","Turret/Dome","Motorized Vari-Focal","2.8-12mm\n(104°-38°)","IP67","40M","PR-JB14IP66 / PR-JB14IP64 / PR-WB-A","Built-in Mic \nD-WDR",null,156]
[1,null,"DI-350A-MVF-G",null,"Pro","Camera HD- 5MP Pro Series,  Dome/Turret IR 40M(3 LED Array), Motorized  2.8-12mm lens, Grey","5MP","Turret/Dome","Motorized Vari-Focal","2.8-12mm\n(84°-32°)","IP67","40M","PR-JB14IP66-G / PR-WB-A-G","D-WDR","EOL, replaced by \nDI-33K0AP-MVF-G",166]
[null,null,"DI-33K0AP-MVF-G",null,"Pro","Camera HD- 5MP Pro Series, Turret IR 40M(3 LED Array), Motorized  2.8-12mm lens Grey","3K","Turret/Dome","Motorized Vari-Focal","2.8-12mm\n(104°-38°)","IP67","40M","PR-JB14IP66-G / PR-WB-A-G","Built-in Mic \nD-WDR","New model",166]
[1,null,"DAI-350A-MVF",null,"Pro","Camera HD-5MP Pro series, Anti-vandal, IR 40M (3LED Array), 2.8-12mm motorized Lens","5MP","Dome Anti-Vandal","Motorized Vari-Focal","2.8-12mm\n(84°-32°)","IP67","40M","PR-JBA14IP66","Anti-Vandal \nD-WDR",null,162]
[1,null,"I2-350A-28  ",null,"Pro","Camera HD- 5MP Pro series, Bullet, IR 20M (1 LED Array), 2.8mm Lens","5MP","Bullet","Fixed","2.8mm\n(91°)","IP67","20M","PR-JB12IP66 / PR-JB12IP64","D-WDR","call for special offer",105]
[1,null,"I2-33K0AP-28",null,"Pro","Camera HD-3K Pro series, 16:9,DWDR,Audio over coax,Bullet, IR 20M , 2.8mm Lens","3K","Bullet","Fixed","2.8mm\n(100°)","IP67","20M","PR-JB12IP66 / PR-JB12IP64","Built-in Mic \nD-WDR",null,103]
[1,null,"I4-350A-28",null,"Pro","Camera HD- 5MP Pro series, Bullet, IR 30M (2LED Array), 2.8mm Lens","5MP","Bullet","Fixed","2.8mm\n(91°)","IP67","40M","PR-JB12IP66 / PR-JB12IP64","D-WDR","call for special offer",122]
[1,null,"I4-33K0AP-28",null,"Pro","Camera HD- 3K Pro series, 16:9,DWDR,Audio over coax,Bullet, IR 40M , 2.8Lens","3K","Bullet","Fixed","2.8mm\n(100°)","IP67","40M","PR-JB12IP66 / PR-JB12IP64","Built-in Mic \nD-WDR",null,120]
[1,null,"I4-350A-VF",null,"Pro","Camera HD- 5MP Pro series, Bullet, IR 40M(3 LED Array), 2.8-12mm Lens","5MP","Bullet","Vari-Focal","2.8-12mm\n(84°-32°)","IP67","40M","PR-JB12IP66 / PR-JB12IP64","D-WDR",null,53.16]
[1,null,"I4-33K0AP-MVF",null,"Pro","Camera HD- 3K Pro series, 16:9,DWDR,Audio over coax,Bullet, IR 40M , 2.8-12mm motorized Lens","3K","Bullet","Motorized Vari-Focal","2.8-12mm\n(103°-38°)","IP67","40M","PR-JB12IP66 / PR-JB12IP64","Built-in Mic \nD-WDR",null,162]
[1,null,"DI-380A-28",null,"Pro","Camera HD- 8MP Pro series, Dome/Turret, IR 20M (1 LED Array), 2.8mm Lens","8MP","Turret/Dome","Fixed","2.8mm\n(89.3°)","IP67","20M","PR-JB12IP66 / PR-JB12IP64 / PR-WB-A","None","Announcing EOL",168]
[1,null,"DI-380A-MVF",null,"Pro","Camera HD- 8MP Pro series, Dome/Turret, IR 40M (3 LED Array), 2.8-12mm motorized Lens","8MP","Turret/Dome","Motorized Vari-Focal","2.8-12mm\n(78°-31.3°)","IP67","40M","PR-JB14IP66 / PR-JB14IP64 / PR-WB-A","None",null,230]
[1,null,"DAI-380A-MVF",null,"Pro","Camera HD-8MP Pro series, Anti-vandal, IR 40M (3LED Array), 2.8-12mm motorized Lens","8MP","Dome Anti-Vandal","Motorized Vari-Focal","2.8-12mm\n(83.5°-32°)","IP67","40M","PR-JB14IP66","Anti-Vandal","call for special offer",255]
[1,null,"I2-380A-28",null,"Pro","Camera HD- 8MP Pro series, Bullet, IR 20M (1 LED Array), 2.8mm Lens","8MP","Bullet","Fixed","2.8mm\n(95°)","IP67","20M","PR-JB12IP66 / PR-JB12IP64","None",null,145]
[1,null,"DS-392A37 ",null,"Pro","Camera, Dummy smoke detector, 3.7mm lens, 1/3  Sensor 2MP  ","2MP","Hidden","Fixed","3.7mm\n(78°)","-","None","None","HLC","Announcing EOL",98]
[1,null,"MC-392A37",null,"Pro","Camera-Hidden,  camera, Fix lens (3.7mm), 1/3\" Sensor, 2MP, 4 in 1,","2MP","Hidden","Fixed","3.7mm\n(78°)","-","None","None","HLC",null,105]
[1,null,"IV-390A37-V2",null,"Pro","Camera, Hidden, Dummy PIR, IR 15M(36 LEDs), 3.7mm lens, 1/3 Sensor, 2MP","2MP","Hidden","Fixed","3.7mm\n(78°)","-","10M","None","HLC",null,98]
[1,null,"DV-320AR-36",null,"Rainbow","Camera HD- 2MP Pro Rainbow series, Turret, IR 20M (1 LED Array), 3.6mm Lens","2MP","Turret/Dome","Fixed","3.6mm\n(84.6°)","IP67","25M","PR-WB-A,\nPR-JB12IP64,\nPR-JB12IP66","Color at night\nBuilt-in Mic\nD-WDR\nHLC",null,89]
[1,null,"BSV-320AR-36",null,"Rainbow","Camera HD- 2MP Pro Rainbow series, Bullet, IR 20M (1 LED Array), 3.6mm Lens","2MP","Bullet","Fixed","3.6mm\n(84.6°)","IP67","25M","PR-JB12IP64,\nPR-JB12IP66","Color at night\nBuilt-in Mic\nD-WDR\nHLC",null,89]
[1]
[1]
[1]
[1]
[1]
[1]
[1]
[1]
[1]
[1]
[1]
[1]

{"sheet":"Access Intercom","index":5,"n_rows":15,"n_cols":5,"rows_kept":15,"cut":false,"hidden":false,"merged":[]}
[]
[]
[]
[]
[]
[null,"Model","Free text","Description","PVP 2025"]
[null,"DB-320WIPN",null,"Video doorbell camera, 2MP.2.3mm Lens,Access control function",309.77549999999997]
[null,"INT-320WIPN",null,"Intercom outdoor station,2MP wifi IPC+3.5inch IPS monitor (NDAA)",619.22249999999997]
[null,"MON-TCH7",null,"Intercom indoor station,7inch touch IPS monitor (NDAA)",354.54]
[null,"MON-TCH7-B",null,"Intercom indoor station,7inch touch IPS monitor (NDAA)- black color",358.50240000000002]
[null,"PR-Chime",null,"Internal chime for Doorbell",55.188000000000002]
[]
[]
[null,"KIT VP","Free text","Description","PVP 2025"]
[null,"PR-VP1","Composed By:                   1x Doorbell (DB-320WIPN),  1x Monitor (MON-TCH7),     1x Switch (PoES-04160C+2I)","Intercom system, 2MP.2.3mm Lens,Access control function",723.89]

{"sheet":"SolarCam","index":6,"n_rows":7,"n_cols":16,"rows_kept":7,"cut":false,"hidden":false,"merged":[]}
[]
[]
[]
[]
["Model","free text","Description","Resolution","Housing","WDR","Lens Type","Lens Focal","Protection","IR range","PSU","Mobile Communication","Special features","Analytic","NDAA","PVP 2025"]
["SOL1-240ADSRN-36",null,"Camera- H.265 S-Sight Series, bullet IR 40M, 3.6mm Lens, 4M with PoE，with solar panel","4MP","Bullet","True WDR","Fixed","3.6mm (92°)","IP65","10-20m","12 VDC ± 25% 60 W ±2Watt On Solar panels","Micro SIM, \nLTE-TDD: Band 38/39/40/41; \nLTE-FDD: Band 1/2/3/4/5/7/8/12/13/18/19/20/25/26/28 \nWCDMA: Band 1/5/8 GSM: Band 2/3/5/8","\nBuilt-in Mic \nBuilt-in speaker\nRed/Blue Strobe Light\nSD Card\nColor at night","Camera Tampering \nStandard- Line Crossing \nStandard- Sterile Area\nDDA- Line Crossing \nDDA- Sterile Area","Yes",2106]
["CEL1-240ADSRN-36",null,"Camera- H.265 S-Sight Series, bullet IR 40M, 3.6mm Lens, 4M with PoE","4MP","Bullet","True WDR","Fixed","3.6mm (92°)","IP65","10-20m","12VDC","Micro SIM, \nLTE-TDD: Band 38/39/40/41; \nLTE-FDD: Band 1/2/3/4/5/7/8/12/13/18/19/20/25/26/28 \nWCDMA: Band 1/5/8 GSM: Band 2/3/5/8","\nBuilt-in Mic \nBuilt-in speaker\nRed/Blue Strobe Light\nSD Card\nColor at night","Camera Tampering \nStandard- Line Crossing \nStandard- Sterile Area\nDDA- Line Crossing \nDDA- Sterile Area","Yes",825]

{"sheet":"PTZ","index":7,"n_rows":37,"n_cols":17,"rows_kept":37,"cut":false,"hidden":false,"merged":[[33,1,33,12],[2,1,2,16],[19,1,19,12],[0,2,0,16],[1,2,1,11],[1,12,1,16]]}
[]
[null,"PTZ"]
[]
[null,"Model","Free Text","Description","Series","Resolution","Housing","WDR","Lens Focal","Power Supply","Protection","IR range","Pan/Tilt Range","Special features","Brackets","NDAA","PVP 2025"]
[null,"I5PT-320IPMX4-P",null,"Camera- IP Bullet IR PTZ, 1080P, X10 with IR 50m distance, with POE","IP","2MP","Bullet","DWDR","2.8-12mm\nX4","12VDC/2A","IP66","50M","250° / 65°","H265","PR-B55JB+","Yes",321]
[null,"I5PT-320IPMX10-P",null,"Camera- IP Bullet IR PTZ, 1080P, X10 with IR 50m distance, with POE","IP","2MP","Bullet","DWDR","5.1-51mm\nX10","12VDC/2A","IP66","50M","250° / 65°","H265","PR-B55JB+","Yes",407]
[null,"MZ-20IPM-2(IR)",null,"IP PTZ,1080P, X20 high speed Pan/Tilt/Zoom camera with IR 80m distance","IP","2MP","Mini\nUltra-Z","DWDR","4.7-97mm\nX20","DC12V/3A","IP66","80M","360° (Endless) / -10°~180° (Auto Flip)","4 Pattern\n8 Scan Route\n8 Cruise Lanes\nVMD","Wall bracket included;\nceiling bracket-PR-B20C ","Yes",610]
[null,"Z4-25IPEN-2(IR)",null,"4\" 2MP x25 PTZ, with DDA Analytics,PoE+, 80°/Sec,120dB WDR, SD Card, wall bracket included","IP","2MP","4''","True WDR","4.8-120mm\nX25\n","PoE+ (802.3at) / DC12V/3A","IP66","100M","360° (Endless) / -5°~185° (Auto Flip)","4 Pattern\n8 Scan Route\n8 Cruise Lanes\nVMD\nAudio In\nAudio Out\nI/O","wall bracket included; \nother brackets- \nPR-CB-Z, \nPR-B50PB, \nPR-B50ECB","Yes",1016]
[null,"Z5-25IPE-2(IR)",null,"5\"2MP x25 PTZ ,DDA Analytics,PoE+,140°/Sec,120dB WDR,SD Card,1Alarm in/out,1Audio in/out, Wall bracket inclued","IP","2MP","5''","True WDR","4.8-120mm\nX25\n","PoE+ (802.3at) / DC24V/3A / AC24V/3A","IP66","150M","360° (Endless) / -3°~183° (Auto Flip)","4 Pattern\n8 Scan Route\n8 Cruise Lanes\nVMD\nAudio In\nAudio Out\nI/O","wall bracket included; \nother brackets- \nPR-CB-Z, \nPR-B50PB, \nPR-B50ECB","No",1150]
[null,"Z3-4ADSN-4",null,"3\"4MPx4 PTZ ,DDA Analytics,PoE+,60°/Sec,120dB WDR,SD Card,1Alarm in/out,1Audio in/out. built-in Mic","IP","4MP","3''","True WDR","2.8-12\nX4","PoE+ (802.3at) / DC12V/2A","IP66","50M","355°  /\n95°","4 Pattern\n8 Scan Route\n8 Cruise Lanes\nVMD\nAudio In\nAudio Out\nI/O","Ceiling bracket included","Yes",527]
[null,"Z4-25IPEN-4(IR)",null,"4\" 4MP x25 PTZ, with DDA Analytics, PoE+, 80°/Sec, 120dB WDR, SD Card,wall bracket included","IP","4MP","4''","True WDR","4.8-120mm\nX25\n","PoE+ (802.3at) / DC12V/3A","IP66","100M","360° (Endless) / -5°~185° (Auto Flip)","4 Pattern\n8 Scan Route\n8 Cruise Lanes\nVMD\nAudio In\nAudio Out\nI/O","wall bracket included; \nother brackets- \nPR-CB-Z, \nPR-B50PB, \nPR-B50ECB","Yes",1198]
[null,"Z5-25IPE-4(IR)",null,"5\"4MP x25 PTZ ,DDA Analytics,PoE+,140°/Sec,120dB WDR,SD Card,1Alarm in/out,1Audio in/out, Wall bracket inclued","IP","4MP","5''","True WDR","4.8-120mm\nX25\n","PoE+ (802.3at) / DC24V/3A / AC24V/3A","IP66","150M","360° (Endless) / -3°~183° (Auto Flip)","4 Pattern\n8 Scan Route\n8 Cruise Lanes\nVMD\nAudio In\nAudio Out\nI/O","wall bracket included; \nother brackets- \nPR-CB-Z, \nPR-B50PB, \nPR-B50ECB","No",1488]
[null,"Z7-37IPEN-4(IR)",null,"4MP 7\" IP PTZ with x37 Zoom, 400m IR LED and AI","IP","4MP","7''","True WDR","6-222mm\nX37\n","PoE+ (802.3at) / DC24V/3A / AC24V/3A","IP67","400M","360° (Endless) /-25°~155° (Auto Flip)","4 Pattern\n8 Scan Route\n8 Cruise Lanes\nVMD\nAudio In\nAudio Out\nI/O","wall bracket included; \nother brackets- \nPR-CB-Z, \nPR-B70PB, \nPR-B70ECB","Yes",3200]
[null,"Z8-37IPEN-4(LS)",null,"4MP 8\" IP PTZ with x37 Zoom, 800m IR Laser and AI","IP","5MP","8''","True WDR","6-222mm\nX37\n","PoE+ (802.3at) / DC24V/3A / AC24V/3A","IP67","800M","360° (Endless) /-25°~155° (Auto Flip)","4 Pattern\n8 Scan Route\n8 Cruise Lanes\nVMD\nAudio In\nAudio Out\nI/O","wall bracket included; \nother brackets- \nPR-CB-Z, \nPR-B70PB, \nPR-B70ECB","Yes",4570]
[null,"I5PT-390AX4",null,"Mini PTZ, bullet IR, 1080P, X4  high speed Pan/Tilt/Zoom bullet camera with IR 50m distance","AHD","2MP","Bullet","-","2.8-12mm\nX4","12VDC/2A","IP66","50M","250° Pan / 65° Tilt","Park Action","PR-B55JB+",null,225]
[null,"I5PT-390AX10",null,"PTZ, bullet IR, 1080P, X10  high speed Pan/Tilt/Zoom bullet camera with IR 50m distance","AHD","2MP","Bullet","-","5.1-51mm\nX10","12VDC/2A","IP66","50M","250° Pan / 65° Tilt","Park Action","PR-B55JB+",null,299]
[null,"MZ-10A-2(IR)",null,"ULTRA-Z, 1080P, 10X high speed Pan/Tilt/Zoom Dome camera with IR","AHD","2MP","Mini\nUltra-Z","-","4.7-47mm\nX10","12VDC/2A","IP66","60M","360° (Endless) / 180° (Auto Flip)","4 Pattern\n4 Auto Scan\n8 Group","wall bracket included",null,555]
[null,"ZE-20A-2(IR)",null,"Eco PTZ, 1080P, 4IN1 X20 high speed Pan/Tilt/Zoom PTZ camera with IR 100m distance, with 220V Power","AHD","2MP","Eco-Z","-","4.9-97mm\nX20","12VDC/2A","IP66","100M","360° (Endless) / 180° (Auto Flip)","4 Pattern\n8 Auto Scan\n4 Group","wall bracket included",null,570]
[null,"ZP-20A-2(IR)",null,"Pro PTZ, 1080P, 4IN1 X20 high speed Pan/Tilt/Zoom PTZ camera with IR 100m distance, with 220V Power","AHD","2MP","Pro-Z","-","4.9-97mm\nX20","24VAC/3A","IP66","100M","360° (Endless) / 180° (Auto Flip)","4 Pattern\n4 Auto Scan\n8 Group\nI/O","wall bracket included",null,755]
[null,"bracket and Accessories"]
[null,"Model","Free Text","Description","PVP 2025"]
[null,"PR-CB-Z",null,"Ceiling pedant mount bracket for PTZ",45.182439791999997]
[null,"PR-ICB-Z",null,"In-Ceiling pedant mount bracket for PTZ Z4 models",58.091708304000008]
[null,"PR-WJB-Z",null,"Bracket- Wall bracket and Junction box  for Z4,Z5,Z6 PTZ",229.46]
[null,"PR-B50PB",null,"Pole mount bracket",52.15]
[null,"PR-B50ECB",null,"External Corner bracket ",50.06]
[null,"PR-B60PB",null,"Pole mount bracket for junction box PR-WJB-Z",154.36000000000001]
[null,"PR-B60ECB",null,"External Corner bracket for junction box PR-WJB-Z",137.68]
[null,"PR-B70PB",null,"Pole mount bracket for Z6 PTZ",75.099999999999994]
[null,"PR-B70ECB",null,"External Corner bracket for Z6 PTZ",62.58]
[null,"PR-B20C",null,"celling bracket for MZ-4 Inch PTZ",32.273171280000007]
[null,"PR-WB-Z3",null,"wall bracket for Z3-4ADSN-4",36.576260783999992]
[null,"PR-WJB-Z3",null,"wall bracket and junction box for Z3-4ADSN-4",73.152521567999983]
[null,"Joystick"]
[null,"Model","Free Text","Description","PVP 2025"]
[null,"IP-Key01-V2",null,"IP controller ",691.01113799999996]
[null,"IP-Key02-V2",null,"Keyboard controller for PTZ and Ossia VMS",914.57356500000003]

{"sheet":"Wi-Fi IP","index":8,"n_rows":9,"n_cols":16,"rows_kept":9,"cut":false,"hidden":false,"merged":[[2,1,2,14],[0,2,0,14],[1,2,1,11],[1,12,1,14]]}
[]
[null,"Wi-Fi\nIP"]
[]
[null,"Model","Free text","Description","Series","Resolution","Housing","WDR","Lens Type","Lens Focal","Protection","IR range","Juntion box","Special features","Analytic","PVP 2025"]
[null,"I3-330WIP536-M",null,"Camera-wireless IPC, 30M (3pcs LED array), 3.6mm lens, 3MP","Special","3MP","Bullet","DWDR","Fix ","3.6mm (90°)","IP66","30M","None","Wireless \nWith WR-04IPC Adapter","None",155]
[null,"WR-04IPC_V2",null,"4ch Repeater for Wi-Fi camera model I3-330WIP536",null,"None","Adapter","None","None","None","None","N/A","Wall Mount","Installation Audio Prompts","None",81.205200000000005]
[null,"I2-340WIPSN-28",null,"Camera-wireless IPC, 20M (6pcs LED array), 2.8mm lens, 4MP, PSU not included",null,"4MP","Bullet","True WDR","Fix ","2.8mm (110°)","IP67","20M","PR-JB12IP66/\nPR-JB12IP65","Wireless \nWithout any Adapter,\nSD Card,\nAudio In","Camera Tampering \nStandard- Line Crossing \nStandard- Sterile Area",209.16]
[null,"PT-848",null,"PnV 4MP Pan/Tilt IP camera with IR, 2.4G&5G, White",null,"4MP","Pan / Tilt","None","Fix ","2.3mm (84°)","None","10M","N/A","Plug & View,\nTwo Way Audio with \nBuilt-in Microphone & \nSpeaker","Motion \nDetection, Human detection",124.18]
[null,"WP-919",null,"1080p PnV Waterproof fix IP camera with IR with EU&US Soket",null,"2MP","Outdoor","None","Fix ","4.0mm","IP66","15M","Wall / \nCeiling Mount Bracket","built-in micorphone \n& speaker","Motion \nDetection",126.31920000000001]

{"sheet":"PoE Switches","index":9,"n_rows":16,"n_cols":11,"rows_kept":16,"cut":false,"hidden":false,"merged":[[0,2,0,9],[1,2,1,8],[2,1,2,9]]}
[]
[null,"PoE Switch  "]
[]
[null,"Model","Free text","Description","Downlink Port","Uplink Port","PoE Power Budget","Power Supply","CCTV MODE","Monitor","PVP 2025"]
[null,"PoES-0460C+2I-V2",null,"4-port 10/100Mbps PoE switch,CCTV Mode, 2-port 10/100Mbps UPLINK ,60W Internal power supply","4ch 10/100","2ch 10/100","60W","100-240VAC","Y","N",75.114810000000006]
[null,"PoES-0460G+1G(HPD)",null,"4+1-port Giga PoE Ethernet Switch, 4 giga ports act as PSE downlink , 1G 55W PD Uplink Port","4ch Giga","1ch Giga","55W","From High Power PoE","N","N",150.22962000000001]
[null,"PoES-0472GC+2G",null,"4+2-Port Giga PoE Ethernet Switch,4 giga Ports act as downlink and uplink,2x1G Port uplink,72W","4ch Giga","2ch Giga","72W","54v/2.2A","Y","N",155.22999999999999]
[null,"PoES-08120C+2I-V2",null,"8-port 10/100Mbps PoE switch, CCTV Mode,2-port 10/100Mbps UPLINK , 120W Internal power supply","8ch 10/100","2ch 10/100","120W","100-240VAC","Y","N",162.41039999999998]
[null,"PoES-08120GC+2GI",null,"8+2 Port Giga PoE Switch,8 giga downlink port, 2 giga uplink port, 120W, with cctv mode","8ch Giga","2ch Giga","120W","100-240VAC","Y","N",186.77195999999998]
[null,"PoES-08120GCL+2Combo",null,"8+2 Port Giga PoE Switch,8 giga downlink port, 2 giga combo port, 120W, with cctv mode,color LCD","8ch Giga","2ch Giga","120W","100-240VAC","Y","LCD",353.24262000000004]
[null,"PoES-16250C+2Combo",null,"16CH unmanaged PoE switch, downlink:*16 100mbps, uplink: *2 1000mbps,total PoE is 250W","16ch 10/100","2ch Combo","250W","100-240VAC","Y","N",466.92990000000003]
[null,"PoES-16250CL+2G+2SFP",null,"16CH unmanaged PoE switch, downlink:*16 100mbps, uplink: *2 1000mbps,total PoE is 250W.CCTV Mode","16ch 10/100","2ch Giga + 2ch SFP","250W","100-240VAC","Y","LCD",649.64159999999993]
[null,"PoES-16250GCL+2SFP",null,"16-Port Giga PoE Ethernet Switch,16 giga Ports act as downlink and uplink,2SFP,250W","16ch Giga","SFP Only +2ch SFP","250W","100-240VAC","Y","LCD",710.54550000000006]
[null,"PoES-24370C+2Combo",null,"24CH unmanaged PoE switch, downlink:*24 100mbps, uplink: *2 1000mbps,total PoE is 370W","24ch 10/100","2ch Combo","370W","100-240VAC","Y","N",527.83000000000004]
[null,"PoES-24370CL+2G+2SFP",null,"24CH unmanaged PoE switch, downlink:*24 100mbps, uplink: *2 1000mbps,total PoE 370W CCTV mode","24ch 10/100","2ch Giga + 2ch SFP","370W","100-240VAC","Y","LCD",812.05200000000002]
[null,"PoES-24370GCL+2SFP",null,"24+2SFPPort Giga PoE Ethernet Switch,24 giga Ports act as downlink and uplink,2xSFP slots,370W","24ch Giga","SFP Only +2ch SFP","370W","100-240VAC","Y","LCD",933.85980000000006]

{"sheet":"PoE Accessories","index":10,"n_rows":13,"n_cols":5,"rows_kept":13,"cut":false,"hidden":false,"merged":[[0,2,0,3],[1,2,1,3],[2,1,2,3]]}
[]
[null,"PoE Accessories"]
[]
[null,"Model","Free text","Description","PVP 2025"]
[null,"PoEI-0130",null,"1 Channel PoE Ethernet Injector IEEE802.3at (30W) ",58.422630000000005]
[null,"PoEI-0160",null,"1 Channel 60W Hi-PoE Ethernet Injector, IEEE80",133.53744]
[null,"PoEI-0190",null,"1 channel 90W PoE Injector, IEEE80.",116.84526000000001]
[null,"PoESP-0124W",null,"1 Channel PoE Ethernet Splitter, IEEE802.3at (24W)",50.076540000000001]
[null,"PoESP-0172W",null,"1 Channel PoE Ethernet + DC ( 24VDC / 3A) Splitter, \nIEEE802.3at (72W), DC Jack / Terminal Connector Output",125.19135000000001]
[null,"PoER-01",null,"1 Channel 10/100M PoE Extender (Repeater), IEEE802.3at",100.15308]
[null,"PoER-02",null,"1 to 2 Channels 10/100M PoE Extender (Repeater), IEEE802.3at",112.67221500000001]
[null,"EOC-01",null,"Set-Transmitter + Receiver, \nEthernet Over Standard Coax Cable Up To 150 Meter",33.384360000000001]
[null,"DCoE-01",null,"Set-Transmitter/Receiver, \nTransmit DC Power and Ethernet Over Ethernet Cable,\n50 Meter Working Distance, Not PoE",14.605657500000001]

{"sheet":"Accessories","index":11,"n_rows":87,"n_cols":7,"rows_kept":87,"cut":false,"hidden":false,"merged":[[0,3,0,6],[1,3,1,5],[2,2,2,6],[82,2,82,6],[25,2,25,6],[56,2,56,6],[72,2,72,6],[4,2,4,6],[6,1,6,6],[13,1,13,6]]}
[]
[null,null,"Accessories"]
[]
[null,"קטגוריה","Category","Free text","Model","Description","PVP 2025"]
[null,null,"Lens"]
[null,null,"Lens",null,"02812DCMP-3-V2","Vari-Focal DC Auto Iris 2.8-12mm,3 Mega-Pixel lens",114.8715225]
[null,"Monitors"]
[null,null,"Monitor",null,"TM-434In1-8","4.3 inch AHD/TVI/CVI/CVBS tester with RS485 up to 8MP with EU&US socket",268.374000384]
[null,null,"Monitor",null,"TM-54In1-2","5 inch  AHD/TVI/CVI/CVBS tester with RS485 up to 2MP ",268.374000384]
[null,null,"Monitor",null,"TM-54In1-8","5 inch AHD/TVI/CVI/CVBS tester with RS485. Network and Coax testers. Up to 8MP with EU&US socket",424.92550060799999]
[null,null,"Monitor",null,"PR-IPS7-W","7\" standalone LCD Monitor with IPS panel, HDMI&AV&VGA,White shell.",201.28050028800001]
[null,null,"Monitor",null,"PR-IPS10-W","10.1\" standalone LCD Monitor with IPS panel , HDMI&AV&VGA,White shell.",268.374000384]
[null,null,"Monitor",null,"MON-24FHD-BL","24\" standalone LED Monitor with IPS panel , HDMI&VGA,black shell.with PSU",270]
[null,"Power Supply"]
[null,null,"Power Supply",null,"PR-12V1A-A","12V 1A Power Supply ",7.0324999999999998]
[null,null,"Power Supply",null,"PR-12V3A","12V 3A Power Supply ",16.9556]
[null,null,"Power Supply",null,"PR-12V5A","12V 5A Power Supply ",26.054199999999998]
[null,null,"Power Supply",null,"PR-12V5A-4","12V 5A Power Supply with 4 splitter",28.944800000000001]
[null,null,"Power Supply",null,"PR-12V5A-4T","Power supply, DC 12V5A with 4 channel terminal block",30.913900000000002]
[null,null,"Power Supply",null,"PR-5A8CH+","8CH, 12V/5A Profesional power supply with socket",97.184299999999993]
[null,null,"Power Supply",null,"PR-5A8CH-B","8CH, 12V/5A Proffesional power supply with room for backup battery with socket",99.250399999999985]
[null,null,"Power Supply",null,"PR-10A9CH+","9CH, 12V/10A Profesional power supply with socket",136.4693]
[null,null,"Power Supply",null,"PR-10A9CH-B","9CH, 12V/10A Proffesional power supply with room for backup battery with socket",161.28190000000001]
[null,null,"Power Supply",null,"PR-12A16CH+","16CH,12V/12A Profesional power supply with socket",190.22669999999999]
[null,null,"Power Supply",null,"PR-20A16CH(1U)","16CH,12V/20A Proffesional power supply,1u case,with  socket",272.93860000000001]
[null,null,"bracket and Junction box"]
[null,"אביזרים","bracket and Junction box",null,"PR-JB14IP66","Bracket- Junction box for I6-/DI-VF, IP66",38.290985347608]
[null,"אביזרים","bracket and Junction box",null,"PR-JB14IP66-G","Bracket- Junction box for I6-/DI-VF, IP66,Grey",38.290985347608]
[null,null,"bracket and Junction box",null,"PR-DJB14IP66","Bracket- Waterproof Junction Box for Large dome / Eyeball , IP66",38.290985347608]
[null,null,"bracket and Junction box",null,"PR-JB14IP64","Bracket- Junction box for I6-/DI-VF, IP64",20.810318123699997]
[null,"אביזרים","bracket and Junction box",null,"PR-JB12IP66","Bracket- Junction box for I4-/I2-/DI-Fix, IP66",34.128921722867993]
[null,"אביזרים","bracket and Junction box",null,"PR-JB12IP66-G","Bracket- Junction box for I4-/I2-/DI-Fix, IP66,Grey",34.128921722867993]
[null,null,"bracket and Junction box",null,"PR-DJB12IP66","Bracket- Waterproof Junction Box for Small dome / Eyeball , IP66",34.128921722867993]
[null,null,"bracket and Junction box",null,"PR-JB12IP64","Bracket- Junction box for I4-/I2-/DI-Fix, IP64",18.313079948856]
[null,"אביזרים","bracket and Junction box",null,"PR-WB14","Bracket- L shape bracket with PR-JB14IP66 for I6-/DI-VF/DAI-VF, IP66",45.78269987214]
[null,"אביזרים","bracket and Junction box",null,"PR-WB12","Bracket- L shape bracket with PR-JB12IP66 for I4-/I2-/DI-Fix/DAI-Fix, IP66   ",45.78269987214]
[null,"אביזרים","bracket and Junction box",null,"PR-WB-A","Bracket- Wall braket for DI-VF, DI-Fix, DAI-Fix, DMA",36.626159897712]
[null,"אביזרים","bracket and Junction box",null,"PR-WB-A-G","Bracket- Wall bracket for DI-VF, DI-Fix, DAI-Fix, DMA.Grey",36.626159897712]
[null,"אביזרים","bracket and Junction box",null,"PR-CB14","Bracket- Straight bracket with PR-JB14IP66 for I6-/DI-VF/DAI-VF, IP66",49.944763496879993]
[null,"אביזרים","bracket and Junction box",null,{"$f":"'[2]Full Pricelist'!$E$269","v":"PR-CB12"},"Bracket- Straight bracket with PR-JB12IP66 for I4-/I2-/DI-Fix/DAI-Fix, IP66   ",49.944763496879993]
[null,"אביזרים למצלמות ממונעות","bracket and Junction box",null,"PR-ICB21","Bracket- In-celling mount bracket for  DAI-fix",45.78269987214]
[null,"אביזרים למצלמות ממונעות","bracket and Junction box",null,"PR-ICB23","Bracket- In-celling mount bracket for  DAI-VF",49.944763496879993]
[null,"אביזרים למצלמות ממונעות","bracket and Junction box",null,"PR-WB50","Bracket- Wall bracket for FEI-",24.972381748439997]
[null,"אביזרים למצלמות ממונעות","bracket and Junction box",null,"PR-CB50","Bracket- Celling bracket for FEI-",19.100163267990002]
[null,"אביזרים למצלמות ממונעות","bracket and Junction box",null,"PR-B10BJB","Junction Box for DMA fix Dome camera (IP Series)",9.3378575976840015]
[null,"אביזרים למצלמות ממונעות","bracket and Junction box",null,"PR-B10EX","Extantion Bracket of 10cm for Junction Box",9.313012800000001]
[null,null,"bracket and Junction box",null,"PR-B20EX","extension Bracket of 20cm",17.694724320000002]
[null,"אביזרים","bracket and Junction box",null,"PR-B42PJB","Smal Plastic junction Box for AHD camera . White color",6.9847596000000003]
[null,"אביזרים","bracket and Junction box",null,"PR-B50PB","Pole mount bracket for PR-JB12xxx, PR-JB14xxx",52.02579530925]
[null,"אביזרים","bracket and Junction box",null,"PR-B50ECB","External Corner bracket for PR-JB12xxx, PR-JB14xxx",49.944763496879993]
[null,"אביזרים","bracket and Junction box",null,"PR-B50JB","Junction Box for Fisheye IP camera",24.972381748439997]
[null,null,"bracket and Junction box",null,"PR-JB1-DB","junction box with roof  for Doorbell",19.100163267990002]
[null,null,"bracket and Junction box",null,"PR-WB15-DB","15 degree bracket for Doorbell",9.3378575976840015]
[null,null,"bracket and Junction box",null,"PR-WJB-INT","Wall mount bracket for INT-320WIPN",37.252051200000004]
[null,null,"bracket and Junction box",null,"PR-IWJB-INT","In-wall junction box for INT-320WIPN",41.908557600000002]
[null,null,"bracket and Junction box",null,"PR-IWJB-MON7","In-wall junction box for MON-TCH7",13.038217919999999]
[null,null,"CONNECTORS"]
[null,"אביזרים","CONNECTORS",null,"PR-C01","BNC Male -RCA female Connector",0.68212368000000012]
[null,"אביזרים","CONNECTORS",null,"PR-C02","T Connector - BNC Female to 2 BNC female",0.94]
[null,"אביזרים","CONNECTORS",null,"PR-C03","T Connector - BNC Male to 2 BNC female",0.85]
[null,"אביזרים","CONNECTORS",null,"PR-C04","BNC female to RCA male",0.64]
[null,"אביזרים","CONNECTORS",null,"PR-C07","BNC Female to BNC Female (BNC Cable Exstender)",0.64]
[null,"אביזרים","CONNECTORS",null,"PR-C08","DC jack male",0.64]
[null,"אביזרים","CONNECTORS",null,"PR-C09","DC jack female",0.64]
[null,"אביזרים","CONNECTORS",null,"PR-C10","DC cable Male (25cm)",0.64]
[null,"אביזרים","CONNECTORS",null,"PR-C11","DC cable female (15cm)",0.64]
[null,"אביזרים","CONNECTORS",null,"PR-C12","Male BNC angular type connector (screwing)",0.64]
[null,"אביזרים","CONNECTORS",null,"PR-C13","BNC Plug (3  pc's in set -use with ratchet BNC carmping tool",0.64]
[null,"אביזרים","CONNECTORS",null,"PR-C14","4CH DC splitter(1 female to 4 male) cable",2.56]
[null,"אביזרים","CONNECTORS",null,"PTR-101V-HD-8","1 CH HD Passive Video Balun Set, 8MP",6.82]
[null,null,"CONNECTORS",null,"PTR-102VP-HD-8","1 CH Passive Balun HD Video And Power - Set,up to 8MP",19.18]
[null,"אביזרים","CONNECTORS",null,"PTR-103VHP-HD","1-ch HD passive video & power balun, 24/36VDC Input. converts to 12VDC at camera side.",29.84]
[null,null,"HDMI"]
[null,"HDMI אביזרים","HDMI",null,"PR-HDMItoVGA","HDMI to VGA converter",13.642473600000002]
[null,"HDMI אביזרים","HDMI",null,"PR-HDEx(4K)","4K HDMI Repeater (Up to 50M)",14.921455500000002]
[null,"HDMI אביזרים","HDMI",null,"PR-SP102(4K)","1 in 2 out 4K HDMI Splitter plastic, black",23.4480015]
[null,"HDMI אביזרים","HDMI",null,"PR-SP104(4K)","1 in 4 out 4K HDMI Splitter, support 3D, with US socket",44.764366500000008]
[null,"HDMI אביזרים","HDMI",null,"PR-SW301(4K)","3 in 1 out HDMI Switch 4k(3840*2160), plastic",21.316365000000005]
[null,"HDMI אביזרים","HDMI",null,"PR-4IN1-Con","Converter- AHD/TVI/CVI/CVBS  to HDMI/VGA/AV , support up to 5MP",136.424736]
[null,"HDMI אביזרים","HDMI",null,"PR-HDoNet+","HDMI over network, extend 40-60 meters",98.055279000000013]
[null,"HDMI אביזרים","HDMI",null,"PR-HDoNet-E","HDMI over network, extend 10-20meters",34.106183999999999]
[null,"HDMI אביזרים","HDMI",null,"PR-HDKVMoNet","HDMI over cat5/5e/6 kvm +2USB with IR",315.48220200000003]
[null,null,"Others"]
[null,null,"Speaker",null,"PR-HS30W","30W 12V-24V active horn speaker with 3.5mm stereo male sound input, Vol control,",196.11055800000003]
[null,null,"Video Server",null,"DVS-IP5-4","video server, H.265 4MP AHD, PoE, audio, alarm, SD, RS-485",330]
[null,null,"Alarm Unit",null,"I/O-1606","USB Alarm Expansion Box, 16CH alarm input, 6CH alarm output",115.64]
[null,null,"Chime",null,"PR-Chime","Internal chime for Doorbell",64.38600000000001]

{"sheet":"מערכת SHOB ","index":12,"n_rows":29,"n_cols":10,"rows_kept":29,"cut":false,"hidden":true,"merged":[[28,3,28,7],[5,3,5,7],[9,9,9,10],[10,9,10,10],[11,9,11,10],[12,9,12,10],[4,1,27,1],[7,3,15,3],[6,9,7,10],[0,1,3,2],[0,3,3,8],[13,9,13,10],[14,9,14,10],[15,9,15,10],[16,9,16,10]]}
[null,"כותרת שו\"ב החדשה"]
[]
[]
[]
[]
[null,null,null,"מחירון שרת "]
[null,null,null,"פריט","מכיל","מחיר","כמות","סה\"כ",null," חויית משתמש 2020"]
[null,null,null,"ערכת בסיס","16 מצלמות",8750,null,{"$f":"F8*G8","v":0}]
[null,null,null,null,"32 גלאים"]
[null,null,null,null,"4 דלתות",null,null,null,null,"ממשק משתמש עשיר וידידותי"]
[null,null,null,null,"ממשק מפות",null,null,null,null,"הגדרת תרחישים פשוטה ויעילה"]
[null,null,null,null,"ממשק תרחישים",null,null,null,null,"הפקת דו\"ח אביזרים תקולים"]
[null,null,null,null,"יומן אירועים",null,null,null,null,"ממשק לכל המערכות הקיימות בשוק"]
[null,null,null,null,"מודולי שליטה",null,null,null,null,"ממשק מפות ויומן אירועים חי ואינטרקטיבי"]
[null,null,null,null,"2 הרשאות לעמודת עבודה",null,null,null,null,"פתרונות ייעודיים לפי דרישה"]
[null,null,null,null,"חומרה עליה מותקנת השו\"ב - לא נועד לצפית וידאו",null,null,null,null,"צוות פיתוח ישראלי זמין"]
[null,null,null,"הרשאה לעמדת עבודה נוספת","תוכנה בלבד",1750,null,{"$f":"F17*G17","v":0}]
[null,null,null,"הוספת קבוצת 8 דלתות ","הרשאה",1750,null,{"$f":"F18*G18","v":0}]
[null,null,null,"הוספת קבוצת 16 מצלמות ","הרשאה",1750,null,0]
[null,null,null,"הוספת קבוצת 32 גלאים","הרשאה",1750,null,0]
[null,null,null,"מודול לשליחת הודעות SMS","כולל מודם, לא כולל SIM",2500,null,0]
[null,null,null,"התקנת הספק","עלות של מערך החבילה 10% לא פחות מ 4000",null,null,0]
[null,null,null,"בניית מסך גרפי (מפה)","עלות בניית מפה אחת",850,null,0]
[null,null,null,"שרות שנתי","החל מהשנה שניה",0.15,null,{"$f":"SUM(H8,H17:H23)*F24","v":0}]
[null,null,null,"עלות מפתח","יום עבודה",1750,null,0]
[null,null,null,"סה\"כ עלות ללא שרות שנתי",null,null,null,{"$f":"SUM(H8,H17:H23)","v":0}]
[]
[]
[null,null,null,"לפרטים נוספים והצעת מחיר: שגיא 09-7601346 שלוחה 217 / 050-5738835"]

{"sheet":"VMS Hardware","index":13,"n_rows":11,"n_cols":6,"rows_kept":11,"cut":false,"hidden":false,"merged":[[0,2,0,5],[1,2,1,4],[2,1,2,5]]}
[]
[null,"VMS Hardware"]
[]
[null,"Category","Model","Free text","Description","PVP 2024 "]
[null,"License","OC-CH",null,"Basic system- 32 ch free \n33-150ch- 18$ per channel\n151-300ch- 15$ per channel\n301ch and up- 12$ per channel","SOB CONSULTA"]
[null,"Management Server- S","OC-MSCL-S(DT)-V2",null,"Ossia VMS Management Server include 256 Licenses/\nClient for OC-MS-XL(1U)  /OC-MSCL-S(DT) servers",3686.39]
[null,"Management Server- M","OC-MS-M(1U)",null,"Ossia VMS Management Server include 512 Licenses ",7099.71]
[null,"Management Server- XL","OC-MS-XL(1U)-V2",null,"Ossia VMS up to 10,000ch Management Server include 512ch Licenses",17070.3]
[null,"Recording Server","OC-RS-16(3U)",null,"Ossia VMS 16HDD Recording Server with Raid and 2 PSU",20520]
[null,"Decoder","DEC-0104N(1U)",null,"IP Decoder, 1*HDMI input 1080P, 4*HDMI output (2*4K+ 2*1080P),1U case",1660.6]
[null,"Joystick","IP-Key02-V2",null,"Keyboard controller for PTZ and Ossia VMS",949.05]

{"sheet":"Maitainance file","index":14,"n_rows":25,"n_cols":42,"rows_kept":25,"cut":false,"hidden":false,"merged":[[0,0,0,6],[0,10,0,16],[0,20,0,26],[0,30,0,36]]}
["IPC",null,null,null,null,null,null,null,null,null,"HDC",null,null,null,null,null,null,null,null,null,"NVR",null,null,null,null,null,null,null,null,null,"DVR",null,null,null,null,null,null,null,null,null,null,"Clean"]
["Series","Resolution","Housing","WDR","Lens type","Special features","Analytic",null,null,null,"Resolution","Housing","Lens type",null,null,"Speical feature",null,null,null,null,"No. Of Channels","Max Resolution","HDD","Dry Contact",null,"Special Feature",null,null,null,null,"Number of Channels","No. of IP Channels","HD Max Resolution","HD Max Real-Time Resolution","HDD","Audio","Dry Contact",null,null,null,null,"Model search"]
["F","H","I","J","K","P","Q",null,null,null,"G","H","I",null,null,"N",null,null,null,null,"F","G","K","N",null,"O",null,null,null,null,"F","G","H","I","L","N","P"]
["Series","Resolution","Housing","WDR","Lens type","Special features","Analytic",null,null,null,"Resolution","Housing","Lens type",null,null,"Speical feature",null,null,null,null,"No. Of Channels","Max Resolution","HDD","Dry Contact",null,"Special Feature",null,null,null,null,"Number of Channels","No. of IP Channels","HD Max Resolution","HD Max Real-Time Resolution","HDD","Audio","Dry Contact"]
["B-Sight","2MP","Bullet","DWDR","Fixed","I/O","Camera Tampering ",null,null,null,"2MP","Bullet","Fixed",null,null,"Anti-vandal",null,null,null,null,4,"5MP","1 of 6TB Max","Based on IPC Only",null,"None PoE",null,null,null,null,4,"up to 2","2MP Lite","1MP","1 of 6TB Max","Based on IPC Only","Based on IPC Only"]
["Eye-Sight","4MP","Turret/Dome","True WDR","Vari-Focal","Audio In","Standard- Line Crossing ",null,null,null,"3K","Turret/Dome","Vari-Focal",null,null,"color at night",null,null,null,null,8,"8MP","1 of 8TB Max","In- 8+IPC Out- 4+IPC",null,"with PoE",null,null,null,null,8,"up to 4","5MP Lite","2MP Lite","1 of 8TB Max","IN- 1+IPC Out- 1","IN- 4+IPC Out- 1"]
["S-Sight","6MP","Fish-Eye",null,"Motorized Vari-Focal","Audio Out","Standard- Sterile Area",null,null,null,"5MP","Box","Motorized Vari-Focal",null,null,"Support WDR",null,null,null,null,16,"12MP","2 of 8TB Max","In- 4+IPC Out- 1+IPC",null,"RAID",null,null,null,null,16,"up to 6","8MP Lite","2MP","2 of 8TB Max","IN- 4+IPC Out- 1+IPC","IN- 4+IPC Out- 1+IPC"]
["Special","8MP","Box",null,"None","SD Card","DDA- Line Crossing",null,null,null,"8MP","Hidden","None",null,null,"D-WDR",null,null,null,null,32,"16MP","8 of 8TB Max","In- 16+IPC Out- 1+IPC",null,"Face",null,null,null,null,32,"up to 8","8MP","4MP Lite","4 of 8TB max","IN- 8+IPC Out- 1","IN- 8+IPC Out- 2+IPC"]
["Smart-Sight","5MP","Hidden",null,null,"Built-in Mic","DDA- Sterile Area",null,null,null,null,"Dome Anti-Vandal",null,null,null,"HLC",null,null,null,null,64,null,"16 of 8TB Max",null,null,"DDA Analytic",null,null,null,null,null,"up to 10",null,"5MP Lite","8 of 8TB Max","IN- 8+IPC Out- 1+IPC","IN- 16+IPC Out- 4+IPC"]
["Rainbow","12MP","Dome Anti-Vandal",null,null,"Built-in Speaker","DDA- Object Counting (line)",null,null,null,null,null,null,null,null,"Built-in Mic",null,null,null,null,128,null,"1 of 10TB Max",null,null,"FishEye",null,null,null,null,null,"up to 12",null,null,"1 of 10TB Max","IN- 16+IPC Out- 1+IPC","IN- 16+IPC Out- 8+IPC"]
[null,null,"Doorbell",null,null,"Wireless","DDA- Object Counting (area)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"2 of 10TB Max",null,null,"2*Ethernet",null,null,null,null,null,"up to 16"]
[null,null,null,null,null,"Color at night","DDA- Loitering Detection",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"8 Of 10TB Max",null,null,"Basic Analytic",null,null,null,null,null,"up to 64"]
[null,null,null,null,null,"Red/Blue Strobe Light","DDA- Illegal Parking Detection",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LPR"]
[null,null,null,null,null,"Check Point Protect","DDA- Audio Exception",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Check Point Protect"]
[null,null,null,null,null,"Wigand","DDA- Area Entry",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AI Engine"]
[null,null,null,null,null,"Wi-Fi","DDA- Area Exit"]
[null,null,null,null,null,"Hybrid Light","DDA2- Advanced Object Classification"]
[null,null,null,null,null,null,"Item monitoring"]
[null,null,null,null,null,null,"Heat Map"]
[null,null,null,null,null,null,"Face Detection "]
[null,null,null,null,null,null,"Face Recognition"]
[null,null,null,null,null,null,"LPR"]
[null,null,null,null,null,null,"Active Deterrence"]
[null,null,null,null,null,null,"Fire Detection"]
[null,null,null,null,null,null,"Temperture alert"]

{"sheet":"Sheet1","index":15,"n_rows":16,"n_cols":3,"rows_kept":16,"cut":false,"hidden":false,"merged":[]}
[]
[null,"Items duties"]
[null,"Cameras",0]
[null,"DVR",0]
[null,"NVR",0]
[null,"Power supply",0]
[null,"Monitor",0.14000000000000001]
[null,"Lens",0]
[null,"Connectors",0]
[null,"UTP Baluns"]
[null,"HOUSING AND BRACKETS",0.06]
[null,"HDMI",0]
[null,"HDD"]
[null,"server",0]
[null,"PoE",0]
[null,"solar",0]